**Connecting the Teledrive to the OPD**

**Connect ribbon cable to drive unit**

**Plug drive unit ‘capsule’ into OPD Rompack**

**Connect drive to power.**

***Light should come on on drive unit and a short ‘blip’ as it tries a drive.***

**Connect power to OPD.**

***OPD goes through initialisation and resets with Invalid Capsule message. Goes through initialisation again and ‘Teledrive 2.0’ appears on bottom left of screen. If this does not appear then initialisation has failed. Go back to start.***

**Put Teletoolkit disc in Drive a: ( left). Press START, 4 ( Applications),2 (Disk Utilities)**

***Should read Drive a:. If it goes to Drive B: then the disc has failed to read properly.***

***Try START 4,4 again.***

**If the disc reads O.K. Screen should show**

**DISK UTILITIES**

1. **Format Disc**
2. **L & R redirection.**
3. **Press 2 to check.**

**Screen shows Change meaning of L from \_\_ to \_\_**

 **Change meaning of R from \_\_ to \_\_**

**Change meaning of to\_\_ to A and B as required.**

**If already A & B then Press f8**

**Press START, 4, 1 ( cartridge menu)**

***Drive A: should read and offer a list of programs***

**Selection includes TELETOOLKIT, LOADER,SHEll and w.h.y. Select TELETOOLKIT.**

***Note: SHELL with reset the OPD.***

**Program should load and offer 1. Disk Utilities.**

**Press 1**

**Enter drive letter required.**

**Screen should change to display disc contents and routines to copy, rename, delete etc.**

**If startup is failing, try a different capsule slot in the Rompack. In the event of a freeze, failure or reset, the teledrive must be connected to the power before the OPD ad the OPD has to log the software in from the ROM in the Teledrive, hence the need to initialise twice.**