DUMP(8)

NAME
dump - incremental file system dump

SYNOPSIS
/etc/dump [ key [ argument ... ] filesystem ]

DESCRIPTION
Dump copies to magnetic tape all files changed after a certain date in the filesystem. The key specifies the date and other options about the dump. Key consists of characters from the set 0123456789fubsdWnc.

0-9 This number is the `dump level'. All files modified since the last date stored in the file /etc/dumpdates for the same filesystem at lesser levels will be dumped. If no date is determined by the level, the beginning of time is assumed; thus the option 0 causes the entire filesystem to be dumped.

f   Place the dump on the next argument file instead of the tape. If the name of the file is ``-'', dump writes to standard output.

u   If the dump completes successfully, write the date of the beginning of the dump on file /etc/dumpdates. This file records a separate date for each filesystem and each dump level. The format of /etc/dumpdates is readable by people, consisting of one free format record per line: filesystem name, increment level and ctime(3) format dump date. /etc/dumpdates may be edited to change any of the fields, if necessary.

b   The blocksize, specified in 1024 byte units, is taken from the next argument. The default is 10 for 800 or 1600 BPI, and 32 for higher densities such as 6250 BPI.

s   The size of the dump tape is specified in feet. The number of feet is taken from the next argument. When the specified size is reached, dump will wait for reels to be changed. The default tape size is 2300 feet.

c   The dump output tape is cartridge tape, not half-inch magtape. Dump will use tape length calculations appropriate for cartridge tape (currently 4000 feet, i.e. 450*9 minus slop) to determine when tapes should be changed. For other length cartridge tapes, use the s option.

d   The density of the tape, expressed in BPI, is taken from the next argument. This is used in calculating the amount of tape used per reel. The default is 1600.

W   Dump tells the operator what file systems need to be dumped. This information is gleaned from the files /etc/dumpdates and /etc/fstab. The W option causes dump to print out, for each file system in /etc/dumpdates the most recent dump date and level, and highlights those file systems that should be dumped. If the W option is set, all other options are ignored, and dump exits immediately.

w   Is like W, but prints only those filesystems which need to be dumped.

n   Whenever dump requires operator attention, notify by means similar to a wall(1) all of the operators in the group “operator”.

If no arguments are given, the key is assumed to be 9u and a default file system is dumped to the default tape.

Dump requires operator intervention on these conditions: end of tape, end of dump, tape write error, tape open error or disk read error (if there are more than a threshold of 32). In addition to alerting all operators implied by the n key, dump interacts with the operator on dump's control terminal at times when dump can no longer proceed, or if something is grossly wrong. All questions dump poses must be answered by typing “yes” or “no”, appropriately.

Since making a dump involves a lot of time and effort for full dumps, dump checkpoints itself at the start of each tape volume. If writing that volume fails for some reason, dump will, with operator permission, restart itself from the checkpoint after the old tape has been rewound and removed, and a new tape has been mounted.

Dump tells the operator what is going on at periodic intervals, including usually low estimates of the number of blocks to write, the number of tapes it will take, the time to completion, and the time to the tape change. The output is verbose, so that others know that the terminal controlling dump is busy, and will be for some time.

Now a short suggestion on how to perform dumps. Start with a full level 0 dump

    dump 0un

Next, dumps of active file systems are taken on a daily basis, using a modified Tower of Hanoi algorithm, with this sequence of dump levels:
3 2 5 4 7 6 9 8 9 9 ... For the daily dumps, a set of 10 tapes per dumped file system is used on a cyclical basis. Each week, a level 1 dump is taken, and the daily Hanoi sequence repeats with 3. For weekly dumps, a set of 5 tapes per dumped file system is used, also on a cyclical basis. Each month, a level 0 dump is taken on a set of fresh tapes that is saved forever.

FILES
/dev/rsd1g	default filesystem to dump from
/dev/rmt8	default tape unit to dump to
/etc/ddate	old format dump date record (obsolete after -J option)
/etc/dumpdates	new format dump date record
/etc/fstab	dump table: file systems and frequency
/etc/group	to find group operator
/tmp/dumplockXXXXXX	lock file

SEE ALSO
restore(8), dump(5), fstab(5)

DIAGNOSTICS
Many, and verbose.

BUGS

Sizes are based on 1600 BPI blocked tape; the raw magtape device has to be used to approach these densities. Fewer than 32 read errors on the filesystem are ignored. Each reel requires a new process, so parent processes for reels already written just hang around until the entire tape is written.

It would be nice if dump knew about the dump sequence, kept track of the tapes scribbled on, told the operator which tape to mount when, and provided more assistance for the operator running restore.