CTAPE(4)

NAME
ctape - cartridge tape pseudo device

DESCRIPTION
The devices ctape0 (rewind) and ctape8 (no rewind) are interfaces to the cartridge tape drive. On SSM-based machines, they are links to rtm0 and rtm8, respectively. On SCED-based machines, they are links to rts0 and rts8, respectively. The ctape links provide a consistent interface to the cartridge tape drive, independent of the machine type. These links are created by /dev/MAKEDEV when invoked with "std", "mtape", or "ctape".

FILES
/dev/ctape*

SEE ALSO
mt(1), ts(4), tm(4), mtape(4), makedev(8)