REMOTE(5)

NAME
remote - remote host description file

DESCRIPTION
The systems known by tip(1C) and their attributes are stored in an ASCII file which is structured somewhat like the termcap(5) file. Each line in the file provides a description for a single system. Fields are separated by a colon (``:''). Lines ending in a \ character with an immediately following newline are continued on the next line.

The first entry is the name(s) of the host system. If there is more than one name for a system, the names are separated by vertical bars. After the name of the system comes the fields of the description. A field name followed by an `=' sign indicates a string value follows. A field name followed by a `#' sign indicates a following numeric value.

Entries named ``tip*'' and ``cu*'' are used as default entries by tip, and the cu interface to tip, as follows. When tip is invoked with only a phone number, it looks for an entry of the form ``tip300'', where 300 is the baud rate with which the connection is to be made. When the cu interface is used, entries of the form ``cu300'' are used.

CAPABILITIES
Capabilities are either strings (str), numbers (num), or boolean flags (bool). A string capability is specified by capability=value; e.g. ``dv=/dev/harris''. A numeric capability is specified by capability#value; e.g. ``xa#99''. A boolean capability is specified by simply listing the capability.

at  (str) Auto call unit type. See the AUTOCALL TYPES section later.

br  (num) The baud rate used in establishing a connection to the remote host. This is a decimal number. The default baud rate is 300 baud.

cm  (str) An initial connection message to be sent to the remote host. For example, if a host is reached through port selector, this might be set to the appropriate sequence required to switch to the host.

cu  (str) Call unit if making a phone call. Default is the same as the `dv' field.

di  (str) Disconnect message sent to the host when a disconnect is requested by the user.

du  (bool) This host is on a dial-up line.

dv  (str) UNIX device(s) to open to establish a connection. If this file refers to a terminal line, tip(1C) attempts to perform an exclusive open on the device to insure only one user at a time has access to the port. Here is an example showing the use of the dv feature with multiple UNIX devices:
    dialout:dv=/dev/ttyh0,/dev/ttyh1,/dev/ttyh2,/dev/ttyh3:

el  (str) Characters marking an end-of-line. The default is NULL. `~' escapes are only recognized by tip after one of the characters in `el', or after a carriage-return.

fs  (str) Frame size for transfers. The default frame size is equal to BUFSIZ.

hd  (bool) The host uses half-duplex communication, local echo should be performed.

ie  (str) Input end-of-file marks. The default is NULL.

oe  (str) Output end-of-file string. The default is NULL. When tip is transferring a file, this string is sent at end-of-file.

pa  (str) The type of parity to use when sending data to the host. This may be one of ``even'', ``odd'', ``none'', ``zero'' (always set bit 8 to zero), ``one'' (always set bit 8 to 1). The default is even parity.

pn  (str) Telephone number(s) for this host. If the telephone number field contains an @ sign, tip searches the file /etc/phones file for a list of telephone numbers; c.f. phones(5).

tc  (str) Indicates that the list of capabilities is continued in the named description. This is used primarily to share common capability information.

Here is a short example showing the use of the capability continuation feature:

UNIX-1200:\
	:dv=/dev/cau0:el=^D^U^C^S^Q^O@:du:at=ventel:ie=#$%:oe=^D:br#1200:
arpavax|ax:\
	:pn=7654321%:tc=UNIX-1200

AUTOCALL TYPES

`at' value
    meaning

biz22f
    BIZCOMP 1022, tone dial

biz22w
    BIZCOMP 1022, pulse dial

biz31f
    BIZCOMP 1031, tone dial

biz31w
    BIZCOMP 1031, pulse dial

df02
    DEC DF02-AC

df03
    DEC DF03-AC

dn11
    DEC DN-11/Able Quadracall

hayes
    Hayes Smartmodem (all models)

ventel
    Ventel 212+

v831
    Vadic 831

v3451
    Vadic 3451

FILES
/etc/remote

SEE ALSO
tip(1C), phones(5)