PLOT(1G)

NAME
plot - graphics filters

SYNOPSIS
plot [ -Tterminal [ raster ] ]

DESCRIPTION
These commands read plotting instructions (see plot(5)) from the standard input, and in general produce plotting instructions suitable for a particular terminal on the standard output.

If no terminal type is specified, the environment parameter $TERM (see environ(7)) is used. Known terminals are:

4014
    Tektronix 4014 storage scope.

450 DASI Hyterm 450 terminal (Diablo mechanism).

300 DASI 300 or GSI terminal (Diablo mechanism).

300S
    DASI 300S terminal (Diablo mechanism).

ver Versatec D1200A printer-plotter. This version of plot places a scan-converted image in `/usr/tmp/raster' and sends the result directly to the plotter device rather than to the standard output. The optional argument causes a previously scan-converted file raster to be sent to the plotter.

FILES
/usr/bin/tek
/usr/bin/t450
/usr/bin/t300
/usr/bin/t300s
/usr/bin/vplot
/usr/tmp/raster

SEE ALSO
plot(3X), plot(5)

BUGS
There is no lockout protection for /usr/tmp/raster.