VAX/VMS V3

|  | Information Research Services | Updated: 30 January 1998

|  |  |  |  | VMS V3 supported three new processors: the VAX-11/750, VAX-11/725, VAX-11/782. V3 features included asymmetric multiprocessing (ASMP) for VAX-11/782, support for new architectures, protocols and busses, system communication architecture (SCS), mass storage control protocol (MSCP), lock management system services, and MONITOR utility for performance monitoring.