MicroVAX II

|  | Information Research Services | Updated: 19 August 1997

|  |  |  |  | The MicroVAX II was based on a single, quad-sized 32-bit processor board and contained the MicroVAX chip (which included memory management). The machine featured a floating-point coprocessor chip, 1MB of on-board memory, Q22-bus interface, Q22-map for DMA transfers, interval timer, boot and diagnostic facility, console serial line unit and time-of-year clock.