
 GEOS hard drive image with joystick support -- October, 2019

 For use with the Trackstar E : the Apple IIe clone on a PC ISA card

 For more disk images, visit...
 www.diskman.com/presents/trackstar

 Special thanks to Breadbox Software for releasing GEOS as freeware.

 GEOS is installed to the hard drive image file PRODOS.HD1 along with
 several productivity applications and some utilities. There's plenty
 of leftover space on the hard drive for your work and document files,
 and to install additional applications.

 To use: 
 
 1). Copy the PRODOS.HD1 file to the same directory as you have installed
     the Trackstar E software ( i.e. C:\STAR ).
 
 2). Execute TSUTILIT.COM and choose "System Configuration" followed by
     "Configure the Disk Drives" to begin the disk drive selection process.

 3). When you get to the options for Slot 7, Drive 1 (aka ProDOS volume),
     select "Drive C" followed by the "DO NOT RESIZE" option. DO NOT rename
     the PRODOS.HD1 file or it will not be discovered by the configuration
     program!

 4). Save your settings and exit the program. Then, execute STAR.COM and
     choose to boot from PRODOS Volume-1. Et viol…, GEOS will boot!

 5). Dismiss and ignore the warning message, "No interrupt source found."
     GEOS is pre-configured to use the Apple joystick connected to your
     Trackstar E. Alternatively, you may use keyboard commands. Enjoy!

 Notes:

 1). GEOS is designed to run on monochrome displays. As the Trackstar E
     defaults to full color, you should press F2 after booting GEOS, to
     automatically switch the display to monochrome mode.
 
 2). The AppleMouse is not compatible with the Trackstar E. You may not
     use the AppleMouse with GEOS or any other Apple II program.
