RTM154 V1.0
;New text
;*****************************************************************************
;*                       << Panasonic KX-P3124 >>                            *
;*                          COMMAND REFERENCE                                *
;*****************************************************************************


;                     *********************************
;                     *****  EPSON Mode Commands  *****
;                     *********************************


<PRINT QUALITY>
Selects print quality.

	Name:   ESC     x       n
	Dec.:   27      120     n
	Hex.:   1B      78      n

	Comments:
	*The following values of n can be used:
		n=0:Draft font
		n=1:LQ font
		n=2:SLQ mode (Roman 5, 10 , 6 and 12 CPI fonts only)
	*PANEL LOCK in the Function mode affects this command.

<FONT STYLE>
Selects LQ font style.

	Name:   ESC     k       n
	Dec.:   27      107     n
	Hex.:   1B      6B      n

	Comments:
	*The following values of n can be used:
		n=0:    Roman 
		n=1:    Sans Serif
		n=2:    Courier 
		n=3:    Prestige 
		n=4:    Script 
		n=5:    OCR-B 
		n=6:    Bold PS 
		n=7:    Orator
	*This command is effective only in letter quality mode (ESC+x+1).
	*PANEL LOCK in the Function mode affects this command.

<SUB/SUPERSCRIPT FONT>
Selects sub/superscript font with characters printed in the
lower/upper area of the line.

	Set:
	Name:   ESC     S       n
	Dec.:   27      83      n
	Hex.:   1B      53      n

	Release:
	Name:   ESC     T
	Dec.:   27      84
	Hex.:   1B      54

	Comments:
	*The following values of n can be used:
		n=0:    Superscript
		n=1:    Subscript
	*Sub/superscript font is 2/3 normal character height.
	*In draft mode, font is normal character width.
	*In LQ mode, font is 2/3 normal fixed character width.
	*In PS mode, font is 2/3 normal PS character width.

<SELECTS FONT BY PITCH AND POINT>
Selects font by pitch and point size

	SET :
	NAME:   ESC     X       m       n1      n2
	Hex.:   1B      58      m       n1      n2
	Dec.:   27      88      m       n1      n2

	Comments:
	*Parameter range:
		0<=m<=127 except 2,3 and 4
			m=0  no change to character spacing
			m=1  character spacing is set to PS
			m>4  set character spacing to 360/m CPI
		0<=n1<=255
		0<=n2<=127
			n1 and n2=0 no change to point size

	*Total points = (n1 + n2 x 256) / 2
		
	Comments:
	*This command overrides the current pitch setting.
	*Only the following point sizes are available: From 8 to 96
	 (in increments of 2) and 10.5 ,21 points.
	*Selecting a combination of 15 CPI and 10 or 20 point characters
	 results in 15-CPI ROM characters being chosen; the height of these 
	 characters is about 2/3 that of normal characters.  Select the pitch 
	 with the ESC+c command to obtain normal height 10 or 20-point
	 characters at 15 CPI.
	*During multipoint mode the printer ignores the ESC+W,ESC+w,ESC+SP,SI,
	 ESC+SI,SO, and ESC+SO commands.
	*The following commands cancel multipoint mode, returning the printer
	 to 10.5-point characters: ESC+P,ESC+M,ESC+g,ESC+p,ESC+!, and ESC+@.

<PICA PITCH>
Sets printing to 10 characters per inch (up to 90 characters per line).

	Name:   ESC     P
	Dec.:   27      80
	Hex.:   1B      50

	Comments:
	*When pica and compressed are set simultaneously, output is
	 17 CPI (up to 153 CPL).
	*PANEL LOCK in the Function mode affects this command.

<ELITE PITCH>
Sets printing to 12 characters per inch (up to 108 characters per line).

	Name:   ESC     M
	Dec.:   27      77
	Hex.:   1B      4D

	Comments:
	*When elite and compressed are set simultaneously, output is
	 20 CPI (up to 180 CPL).
	*PANEL LOCK in the Function mode affects this command.

<MICRON PITCH>
Sets printing to 15 characters per inch (up to 135 characters per line).

	Name:   ESC     g
	Dec.:   27      103
	Hex.:   1B      67

	Comments:
	*When micron and compressed are set simultaneously, output is
	 15 CPI (up to 135 CPL).
	*PANEL LOCK in the Function mode affects this command.

<COMPRESSED PITCH>
Sets printing to 17 characters per inch (up to 153 characters per line).

	Set:
	Name:   SI      or      ESC     SI
	Dec.:   15      or      27      15
	Hex.:   0F      or      1B      0F

	Release:
	Name:   DC2
	Dec.:   18
	Hex.:   12

	Comments:
	*When pica and compressed are set simultaneously, output is
	 17 CPI (up to 153 characters per line).
	*When elite and compressed are set simultaneously, output is
	 20 CPI (up to 180 CPL).
	*When micron and compressed are set simultaneously, output is
	 15 CPI (up to 135 CPL).
	*When PS (Proportional Spacing) and compressed are set
	 simultaneously, font is compressed PS character width.
	*PANEL LOCK in the Function mode affects this command.

<PROPORTIONAL SPACING>
Sets proportional spacing between characters.

	Set:
	Name:   ESC     p       1
	Dec.:   27      112     1
	Hex.:   1B      70      01

	Release:
	Name:   ESC     p       0
	Dec.:   27      112     0
	Hex.:   1B      70      00

	Comments:
	*Proportional spacing overrides pica, elite, and micron
	 pitch setting.
	*When PS (Proportional Spacing) and compressed are set
	 simultaneously, font is compressed PS character width.
	*This command is effective only in letter quality mode (ESC+x+1).
	*PANEL LOCK in the Function mode affects this command.

<PROGRAMMABLE PITCH/HIGHLIGHTING>
Sets a combination of character pitch and/or highlighting.

	Name:   ESC     !       n       (n = 0 to 255)DEC
	Dec.:   27      33      n
	Hex.:   1B      21      n

	Comments:
	*The value of n determines the pitch and highlight combinations.
	*To find the value of n, add up the decimal numbers below for
	 the print modes you wish to select:
		  0: Pica
		  1: Elite
		  2: PS
		  4: Compressed
		  8: Emphasized
		 16: Double-strike
		 32: Double-wide
		 64: Italic
		128: Underlining

	*Invalid values of n follow rules noted in individual commands.
	*When elite and compressed are set simultaneously output is
	 20 CPI (up to 180 CPL).
	*PANEL LOCK in the Function mode affects this command.

<EMPHASIZED PRINTING>
Sets printing to twice the original horizontal dot density.

	Set:
	Name:   ESC     E
	Dec.:   27      69
	Hex.:   1B      45

	Release:
	Name:   ESC     F
	Dec.:   27      70
	Hex.:   1B      46

	Comments:
	*Emphasized characters are printed at half speed.
	*PANEL LOCK in the Function mode affects this command.

<DOUBLE HIGH PRINTING>
Sets double high printing.

	Set:
	Name:   ESC     w       1
	Dec.:   27      119     1
	Hex.:   1B      77      01

	Release:
	Name:   ESC     w       0
	Dec.:   27      119     0
	Hex.:   1B      77      00

	Comments:
	*In the pull tractor mode, this command will not reverse feed paper
	 correctly and the resulting printout may not be correct.
	*PANEL LOCK in the Function mode affects this command.

<DOUBLE WIDE PRINTING (SINGLE LINE)>
Sets double wide (expanded) printing for one line only.

	Set:
	Name:   SO      or      ESC     SO
	Dec.:   14      or      27      14
	Hex.:   0E      or      1B      0E

	Release:
	Name:   DC4     or      ESC     W       0
	Dec.:   20      or      27      87      0
	Hex.:   14      or      1B      57      00

	Comments:
	*Single line double wide printing is released when:
	 - a LF, FF or VT is executed.
	 - the printer is initialized.
	 - DC4 or ESC+W+0 is executed.
	 - ESC+!+0 is executed.
	*PANEL LOCK in the Function mode affects this command.

<DOUBLE WIDE PRINTING>
Sets double wide (expanded) printing.

	Set:
	Name:   ESC     W       1
	Dec.:   27      87      1
	Hex.:   1B      57      01

	Release:
	Name:   ESC     W       0
	Dec.:   27      87      0
	Hex.:   1B      57      00

	Comments:
	*DC4 will not release the double wide printing set by ESC+W+1.
	*Expanded pica output is 5 CPI.
	*Expanded elite output is 6 CPI.
	*Expanded micron output is 7.5 CPI.
	*Expanded compressed output is 8.5 CPI.
	*PANEL LOCK in the Function mode affects this command.

<OUTLINE AND SHADOW PRINTING>
Sets outline and shadow printing.

	Name:   ESC     q       n
	Dec.:   27      113     n
	Hex.:   1B      71      n

	Comments:
	*The following values of n can be used.
		n=0: Releases outline/shadow printing
		n=1: Outline
		n=2: Shadow
		n=3: Outline with Shadow
	*PANEL LOCK in the Function mode affects this command.

<DOUBLE STRIKE PRINTING>
Sets double printing.

	Set:
	Name:   ESC     G
	Dec.:   27      71
	Hex.:   1B      47

	Release:
	Name:   ESC     H
	Dec.:   27      72
	Hex.:   1B      48

	Comments:
	*Double strike printing prints each line twice, with the second
	 line slightly below the first to create a bold appearance.
	*PANEL LOCK in the Function mode affects this command.

<UNDERLINING>
Sets continuous underlining of characters.

	Set:
	Name:   ESC     -       1
	Dec.:   27      45      1
	Hex.:   1B      2D      01

	Release:
	Name:   ESC     -       0
	Dec.:   27      45      0
	Hex.:   1B      2D      00

	Comment:
	*Bit image data, spaces set by the HT code, and IBM graphic
	 characters will not be underlined.

<SCORE>
Sets/releases score.

	Name:   ESC     (       -       3       0       1        d1     d2
	Dec.:   27      40      45      3       0       1        d1     d2
	Hex.:   1B      28      2D      03      00      01       d1     d2

	Comments:
	*The value of d1 determines the location of the score:
		d1=1: Underline
		d1=2: Strikethrough
		d1=3: Overscore
	*The value of d2 determines whether the score line is single,
	 double, broken or continuous:
		d2=0: Cancel the score line selected by d1
		d2=1: Single continuous line
		d2=2: Double continuous line
		d2=5: Single broken line
		d2=6: Double broken line

<CHARACTER DOT SPACING>
Sets character dot spacing

	Name:   ESC     SP      n        (n = 0 to 127)DEC
	Dec.:   27      32      n
	Hex.:   1B      20      n

	Comment:
	*Sets the amount of dot space (Draft: n/120 inch,
	 LQ: n/180 inch) added to the right of each character
	 to allow for micro justification.

<UNIT>  
Set unit

	SET :
	NAME:   ESC     (       U       1       0       n
	Hex.:   1B      28      55      1       0       n
	Dec.:   27      40      85      01      00      n

	Comment:
	*Parameter range:
		n = 10,20,30,40,50,60
	*Sets the units for the vertical print position [ ESC(V and ESC(v ],
	 horizontal print position [ ESC\ and ESC $] and page format
	 [ ESC(C and ESC(c ] commands to n/3600 inch.

<HORIZONTAL MOTION INDEX (HMI)>
Set horizontal motion index (HMI)

	SET :
	NAME:   ESC     c       n1      n2
	Hex.:   1B      63      n1      n2
	Dec.:   27      99      n1      n2

	Comment:
	*Parameter range:
		0<=n1<=255
		0<=n2<=4  
		0<(n1 + (n2x256))<=1080 
	*HMI<=3.00 inches

	Notes:
	*Sending this command cancels additional character space set with the 
	 ESC+SP command.
	*The HMI setting made with this command is canceled when the printer
	 receives the following commands: SO,SI,DC2,DC4,ESC+W,ESC+P,ESC+M,
	 ESC+g,ESC+p,ESC+!,ESC+SP, and ESC+@.
	*Use this command to set the pitch if you want to print normal-height 
	 10 or 20-point characters at 15 CPI during multipoint mode. Selecting
	 15 CPI for 10 or 20-point characters with the ESC+X command results in
	 characters being printed at 2/3 their normal height.

<ITALIC FONT>
Selects italic character printing.

	Set:
	Name:   ESC     4
	Dec.:   27      52
	Hex.:   1B      34

	Release:
	Name:   ESC     5
	Dec.:   27      53
	Hex.:   1B      35

	Comments:
	*Italic characters are printed in place of characters
	 in character set locations 32DEC to 126DEC (20 HEX to 7E HEX).
	*This command is effective regardless of character set 
	 selected by ESC+t+n.
	*PANEL LOCK in the Function mode affects this command.

<INTERNATIONAL CHARACTER SET>
Selects international character set.

	Name:   ESC     R       n
	Dec.:   27      82      n
	Hex.:   1B      52      n

	Comments:
	*The following values of n can be used:
		n=0 to 13: Selects one of 14 language character sets.
		n=64     : Selects legal character set.
	*Character set tables in the appendix of the operating instruction
	 manual identifies the characters generated by the appropriate
	 codes.
	*International character sets can be set through the initial setup
	 disk.
	*PANEL LOCK in the Function mode affects this command.

<ENABLE UPPER CONTROL CODES>
Assigns character codes 128 to 159 as control codes

	Name:   ESC     7
	Dec.:   27      55
	Hex.:   1B      37

	Comments:
	*Refer to character set tables in appendix of the operating
	 instruction manual.
	*This command is not operational when the Italic character
	 set is selected by ESC+t+n.
	*PANEL LOCK in the Function mode affects this command.

<ENABLE PRINTING OF UPPER CONTROL CODES>
Assigns character codes 128 to 159 as printable characters

	Name:   ESC     6
	Dec.:   27      54
	Hex.:   1B      36

	Comments:
	*Refer to character set tables in appendix of the operating
	 instruction manual.
	*This command is not operational when the Italic character
	 set is selected by ESC+t+n.

<ALTERNATE CHARACTER TABLE>
Selects alternate character table.

	Name:   ESC     t       n
	Dec.:   27      116     n
	Hex.:   1B      74      n

	Comments:
	*The following values of n can be used:
		n=0: Character table 0 : default = Italic
		n=1: Character table 1 : default = PC437 (US)
		n=2: Character table 2 : default = User defined
		n=3: Character table 3 : default = PC437 (US)
	*Use the ESC ( t command to assign a pre-defined character set
	 to a character table.  The character set charts are found in the         
	 appendix of the operating instruction manual.
	*To copy user-defined characters to the upper half of the character        
	 table use the ESC t 2 command. This command will not work if you 
	 have assigned another character table to table 2.
	*PANEL LOCK in the Function mode affects this command.

<ASSIGN CHARACTER TABLE>
Assign character table

	SET :
	NAME:   ESC     (       t       3       0       n1      n2      n3
	Hex.:   1B      28      74      3       0       n1      n2      n3
	Dec.:   27      40      116     03      00      n1      n2      n3

	Comment:
	*Parameter range:
		0<=n1<=3, 48<=n1<=51
		0<=n2<=255
		n3 = 0
	*n1 specifies the character table to re-assign.
	*n2 specifies the character set to assign to a character table.        
		possible values are:
			0 = Italic                1 = PC437(US)
			3 = PC850(MULTINATIONAL)  5 = PC853(TURKISH)
			7 = PC860(PORTUGAL)       8 = PC863(CANADA-FRENCH)
			9 = PC865(NORWAY)
	*Refer to the character set tables in the appendix of the operating
	 instruction manual.
	*Character tables assigned to tables 0 and 1 with this command are not
	 cleared by the ESC+@ (initialize printer) command.


<PRINT DATA AS CHARACTER>
Print data as characters

	SET :
	NAME:   ESC     (       ^       n1      n2      Data
	Hex.:   1B      28      5E      n1      n2      Data
	Dec.:   27      40      94      n1      n2      Data

	Comment:
	*Parameter range:
		0<=n1<=255
		0<=n2<=127
	 Amount of data to print as characters = n1 + (256*n2).
	*The printer ignores data if no character is assigned to that character
	 code in the currently selected character table.

<8-PIN STANDARD DENSITY GRAPHICS>
Sets standard density graphics mode [60 dots per inch 
(25.4 mm)].

	Name:   ESC     K       n1      n2      Data
	Dec.:   27      75      n1      n2      Data
	Hex.:   1B      4B      n1      n2      Data

	Comment:
	*Refer to "ESC+*+m+n1+n2" command.

<8-PIN DOUBLE DENSITY GRAPHICS>
Sets double density graphics mode [120 dots per inch
(25.4 mm)].

	Name:   ESC     L       n1      n2      Data
	Dec.:   27      76      n1      n2      Data
	Hex.:   1B      4C      n1      n2      Data

	Comment:
	*Refer to "ESC+*+m+n1+n2" command.

<8-PIN DOUBLE SPEED/DOUBLE DENSITY GRAPHICS>
Sets double speed double density graphics mode 
[120 dots per inch (25.4 mm)].

	Name:   ESC     Y       n1      n2      Data
	Dec.:   27      89      n1      n2      Data
	Hex.:   1B      59      n1      n2      Data

	Comments:
	*Horizontal adjacent dots cannot be printed.
	*Refer to "ESC+*+m+n1+n2" command.

<8-PIN QUADRUPLE DENSITY GRAPHICS>
Sets quadruple density graphics mode
[240 dots per inch (25.4 mm)].

	Name:   ESC     Z       n1      n2      Data
	Dec.:   27      90      n1      n2      Data
	Hex.:   1B      5A      n1      n2      Data

	Comments:
	*Horizontal adjacent dots cannot be printed.
	*Refer to "ESC+*+m+n1+n2" command.

<BIT IMAGE MODE SELECTION>
Selects one of the 8-pin or 24-pin bit image graphic modes.

	Name:   ESC     *       m       n1      n2      Data
	Dec.:   27      42      m       n1      n2      Data
	Hex.:   1B      2A      m       n1      n2      Data

	Comments:
	*The following table illustrates the various modes based upon the
	 values of m.

	m    pin  dpi   dpl
	----------------------------------------------------
	 0    8    60    540    Standard Density
	 1    8   120   1080    Double Density
	 2    8   120   1080    Double Speed, Double Density
	 3    8   240   2160    Quadruple Density
	 4    8    80    720    CRT I
	 6    8    90    810    CRT II
	32   24    60    540    Standard Density
	33   24   120   1080    Double Density
	38   24    90    810    CRT III
	39   24   180   1620    Triple Density
	40   24   360   3240    Hex Density

	*When m=2, 3 or 40, horizontal adjacent dots cannot be printed.
	*The values n1 and n2 indicate the number of graphic columns
	 to be printed.

	* Bit Image (Graphics)
	 Bit image (Graphics) is used to produce pictures, graphs, charts
	 or creative patterns. Many commercial software packages use bit
	 images.
	 This printer has six 8-pin bit image modes and five 24-pin bit
	 image modes within Epson mode, and has four 8-pin/24-pin bit image 
	 modes within IBM mode, so that you have a wide variety of image
	 printing. When you use a commercial software package, you should
	 refer to your software instruction manual for the proper use.
	 Each printer mode has its own bit image commands. Because
	 differences between the two modes are few, only Epson mode is used
	 here as an example of how to print bit images through software
	 commands.

	 1. Dot Density

	 Dot density (dot resolution) refers to the maximum number of dots
	 that can be printed in an inch or on a line. This printer enables
	 you to access a variety of dot densities through specific control
	 commands. The various dot densities and corresponding control
	 commands appear as follows:
								    Maximum
     Command              Function                      Dots/Inch  Dots/Line
ESC+"K"+n1+n2           Standard density                     60         540
ESC+"L"+n1+n2           Double density                      120        1080 
ESC+"Y"+n1+n2           Double speed,Double density         120        1080
ESC+"Z"+n1+n2           Quadruple density                   240        2160
ESC+"*"+m+n1+n2         8-Pin Mode Selection:
			 m=0 (Standard)                      60         540
			 m=1 (Double)                       120        1080
			 m=2 (Double speed,Double density)  120        1080
			 m=3 (Quadruple density)            240        2160
			 m=4 (CRT I)                         80         720
			 m=6 (CRT II)                        90         810
			24-Pin Mode Selection:
			 m=32 (Standard)                     60         540
			 m=33 (Double)                      120        1080
			 m=38 (CRT III)                      90         810
			 m=39 (Triple)                      180        1620
			 m=40 (Hex)                         360        3240
ESC+"["+"g"+n1+n2+m     8-Pin Mode Selection:
			 m=0 (Standard)                      60         540
			 m=1 (Double)                       120        1080
			 m=2 (Double speed,Double density)  120        1080
			 m=3 (Quadruple density)            240        2160
			24-Pin Mode Selection:
			 m=8 (Standard)                      60         540
			 m=9 (Double)                       120        1080
			 m=11 (Triple)                      180        1620
			 m=12 (Hex)                         360        3240

	 2. 8-Pin Bit Image Mode
	 This printer has 24 pins in the printhead. The distance between
	 the centers of adjacent pins is 1/180inch (0.14 mm), and the
	 diameter of each pin is 1/127 inch (0.2 mm). In 8-pin bit image
	 mode the 24 pins of the printhead are grouped as follows. One byte
	 is sent to the printer for each column to be printed. Each bit of
	 that byte represents an individual pin-block. By summing the powers
	 of two corresponding to each pin-block you wish to fire, you will
	 obtain a numerical value for the column in question. By sending a
	 string of bytes, numerical values for each column on a line are
	 input and processed. The result is one line of graphics.

	Pin-block  Pin-block Code  Pins  Pin No.  Pin-block Code  Pin-block
	__________________________                __________________________
				     O      1      2^7=128           1      
	   1          2^7=128        O      2     __________________________
	__________________________   O      3     ________________1_and_2___
				     O      4      2^6=64            2      
	   2          2^6=64         O      5     __________________________
	__________________________   O      6      2^5=32            3      
				     O      7     __________________________
	   3          2^5=32         O      8     ________________3_and_4___
	__________________________   O      9      2^4=16            4      
				     O      10    __________________________
	   4          2^4=16         O      11     2^3=8             5      
	__________________________   O      12    __________________________
				     O      13    ________________5_and_6___
	   5          2^3=8          O      14     2^2=4             6      
	__________________________   O      15    __________________________
				     O      16     2^1=2             7      
	   6          2^2=4          O      17    __________________________
	__________________________   O      18    ________________7_and_8___
				     O      19     2^0=1             8      
	   7          2^1=2          O      20    __________________________
	__________________________   O      21     Not used
				     O      22     Not used
	   8          2^0=1          O      23     Not used
	__________________________   O      24     Not used
	Epson mode and IBM mode                  IBM mode
	(Alternate Graphic Mode: ON)             (Alternate Graphic Mode: OFF)


	 Note:
	 In the Epson mode or IBM mode with Alternate Graphic Mode (AGM)
	 set to ON through the initial setup disk, 8-pin bit image graphics
	 is printed by using all 24 pins in the printhead.
	 In IBM mode with Alternate Graphic Mode (AGM) set to OFF, 8-pin
	 bit image graphics is printed by using upper 20 pins in the
	 printhead.

	 As an example, suppose you want to fire pin-blocks 1, 2, 5 and
	 8 simultaneously. Then you compute the following sum:

		Input code = Pin-block 1 code + Pin-block 2 code +
			     Pin-block 5 code + Pin-block 8 code
			   = 2^7 + 2^6 + 2^3 + 2^0
			   = 128 + 64 + 8 + 1
			   = 201

	 Thus, the value 201 is entered in the CHR$ function in order to
	 print a single column of dots resulting from firing pin-blocks
	 1, 2, 5, and 8.

	 For our final example, refer to the standard density designation
	 in Table above. This setting is given by ESC+"K"+n1+n2. To print
	 image graphics, you must specify to the printer how many columns
	 are to be used. This is done by finding values for n1 and n2, as
	 follows:
	 Divide the total number of columns you select, by 256 (max # of
	 columns). The result is n1 and the remainder is n2.


		n1 = 100 MOD 256 = 100
		n2 = 100 / 256   = 0            so, n2=0 and n1=100

	 Our control code ESC+"K"+n1+n2 now translates into:

	 LPRINT CHR$(27)+"K"+CHR$(100)+CHR$(0);

	 If you use ESC+"["+"g"+n1+n2+m in IBM mode, compute the values of
	 n1 and n2 as follows:
		n2 x 256 + n1 = Column x Bytes + 1
		m=0, 1, 2, 3:   Bytes=1
		m=8, 9, 11, 12: Bytes=3

	 For example, 24-pin bit image of 100 column is:
		n2 x 256 + n1 = 100 x 3 + 1 = 301       so, n2=1 and n1=45.

	 For example, you select 100 columns and double density (m=9), so
	 your bytes are equal to 3. Now, use the following equation:
	 100 columns x 3 bytes + 1 = 301 (always add 1).

	 Using the equation from above, we have:
		n1 = 301 MOD 256 = 45
		n2 = 301 / 256   = 1            so, n2=1 and n1=45

	 A programming example is as follows:

	 10 REM STANDARD DENSITY
	 20 WIDTH "LPT1:",255
	 30 OPEN "LPT1:" AS #1
	 40 PRINT #1,CHR$(27)+"3"+CHR$(24);
	 50 PRINT #1,CHR$(27)+"K"+CHR$(100)+CHR$(0);
	 60 FOR I=1 TO 5
	 70 PRINT #1,CHR$(1)+CHR$(2)+CHR$(4)+CHR$(8)+CHR$(16);
	 80 PRINT #1,CHR$(32)+CHR$(64)+CHR$(128)+CHR$(64)+CHR$(128);
	 90 PRINT #1,CHR$(64)+CHR$(128)+CHR$(64)+CHR$(128)+CHR$(64);
	 100 PRINT #1,CHR$(32)+CHR$(16)+CHR$(8)+CHR$(4)+CHR$(2);
	 110 NEXT I
	 120 PRINT #1,CHR$(13)+CHR$(10);
	 130 PRINT #1,CHR$(27)+"K"+CHR$(100)+CHR$(0);
	 140 FOR I=1 TO 5
	 150 PRINT #1,CHR$(128)+CHR$(64)+CHR$(32)+CHR$(16)+CHR$(8);
	 160 PRINT #1,CHR$(4)+CHR$(2)+CHR$(1)+CHR$(2)+CHR$(1);
	 170 PRINT #1,CHR$(2)+CHR$(1)+CHR$(2)+CHR$(1)+CHR$(2);
	 180 PRINT #1,CHR$(4)+CHR$(8)+CHR$(16)+CHR$(32)+CHR$(64);
	 190 NEXT I
	 200 PRINT #1,CHR$(13)+CHR$(10);
	 210 CLOSE
	 220 END

	 Note:
	 Line 20 and 30 are necessary for the proper execution of this
	 program on many IBM-compatible computers.

	 Line 40 is necessary to set the line feed for printing in the
	 bit image mode. In the IBM mode, when AGM is set to OFF through
	 the initial setup disk, it will amount to 24/216inch.


	 3. 24-Pin Bit Image Mode
	 In the 24-pin bit image mode, all 24-pins of the printhead may
	 be fired. In this mode, 3 data bytes must be sent to the printer
	 for each column. The 24 pins in the printhead are divided into
	 three portions, the upper 8 pins, middle 8 pins and lower 8 pins.
	 As an example, suppose you want to fire pins 1, 2, 5, 8, 9, 11, 12,
	 21 and 24 simultaneously. Then you compute the following three
	 values:

	 Byte 1: Input code=Pin 1 code+Pin 2 code+Pin 5 code+Pin 8 code
			   =2^7 + 2^6 + 2^3 + 2^0 = 128 + 64 + 8 + 1 
			   = 201
	 Byte 2: Input code=Pin 9 code+Pin 11 code+Pin 12 code
			   =2^7 + 2^5 + 2^4 = 128 + 32 + 16
			   = 176
	 Byte 3: Input code=Pin 21 code+Pin 24 code
			   =2^3 + 2^0 = 8 + 1
			   = 9

	 Thus, the three bytes for a single column of dots are entered as
	 CHR$(201);CHR$(176);CHR$(9); Refer to the 24-pin standard density
	 command. This setting is given by ESC+"*"+m+n1+n2, where m=32.
	 Suppose you wish to print 100 columns of dots, where every column
	 fires pins 1, 2, 5, 8, 9, 11, 12, 21 and 24 as above.

	 As in the 8-pin example, n1=100 and n2=0. Our command
	 ESC+"*"+m+n1+n2 now translates into 
	 LPRINT CHR$(27)+"*"+CHR$(32)+CHR$(100)+CHR$(0);
	 If we incorporate this information into a program, we might have
	 the following:

	 10 REM 24 PIN STANDARD DENSITY
	 20 WIDTH "LPT1:",255
	 30 OPEN "LPT1:" AS #1
	 40 PRINT #1,CHR$(27)+"*"+CHR$(32)+CHR$(100)+CHR$(0);
	 50 FOR I=1 TO 100
	 60 PRINT #1,CHR$(201);
	 70 PRINT #1,CHR$(176);
	 80 PRINT #1,CHR$(9);
	 90 NEXT I
	 100 PRINT #1,CHR$(13)+CHR$(10);
	 110 CLOSE
	 120 END

	 Note:
	 If in IBM mode, AGM must be set to ON.

	 If you use ESC+"["+"g"+n1+n2+m in IBM mode, you must change
	 line 40 as follows:
	 40 PRINT #1, CHR$(27)+"["+"g"+CHR$(45)+CHR$(1)+CHR$(8);

	 Bit Image Graphics prints uni-directional for high precision
	 printing. For high speed printing set the printer to bi-directional
	 printing through initial setup mode or through the initial setup
	 disk.

	 Graphics mode is released immediately following the printing of
	 all bit image data. Printing will return to text mode.

	 Bit image data is not affected by MSB control commands.


	 4. Alternate Graphic Mode (AGM)
	 There are two methods of graphic printing in IBM mode. You can
	 set them through Alternate Graphic Mode setting through the initial
	 setup disk.

	 When AGM is set to OFF, 8-pin bit image graphic is printed by
	 using pins 1 through 20.

	 When AGM is set to ON, the printing of 8-pin graphic mode is the
	 same as in Epson mode. Also, graphic printing command, ESC+"*" in
	 Epson mode is effective in this mode. Therefore, you can use the
	 same command as in Epson mode.

	The following table shows commands affected by AGM mode.

				  AGM ON                  AGM OFF
ESC+"K"+n1+n2                   use 24 pin              use 20 pin
ESC+"L"+n1+n2                   use 24 pin              use 20 pin
ESC+"Y"+n1+n2                   use 24 pin              use 20 pin
ESC+"Z"+n1+n2                   use 24 pin              use 20 pin

ESC+"["+"g"+    8-pin mode      use 24 pin              use 20 pin
 n1+n2+m       24-pin mode      use 24 pin              use 24 pin

ESC+"3"+n                       based on 1/180 inch     based on 1/216 inch
ESC+"A"+n                       based on 1/60 inch      based on 1/72 inch
ESC+"J"+n                       based on 1/180 inch     based on 1/216 inch


<BIT IMAGE MODE REASSIGNMENT>
Reassigns bit image graphics mode density.

	Name:   ESC     ?       n       m
	Dec.:   27      63      n       m
	Hex.:   1B      3F      n       m

	Comments:
	*The value of n specifies the graphics mode which is
	 to be reassigned:
		n=75: Reassign Standard Density (ESC+K+n1+n2)
		n=76: Reassign Double Density (ESC+L+n1+n2)
		n=89: Reassign Double Speed, Double Density (ESC+Y+n1+n2)
		n=90: Reassign Quadruple Density (ESC+Z+n1+n2)
	*The value of m specifies the graphics mode to which the
	 original is to be reassigned. Refer to the table in the 
	 <BIT IMAGE MODE SELECTION> section for values of m.


<GRAPHIC MODE>
Select graphics mode

	SET :
	NAME:   ESC     (       G       1       0       n
	Hex.:   1B      28      47      1       0       n
	Dec.:   27      40      71      01      00      n

	Comment:
	*Parameter range:
		n = 1,49

	Notes:
	*Exit graphics mode by sending the ESC+@ (Initialize printer) command.
	*This command clears all user-defined characters and tab settings.
	*Text printing is not possible during graphics mode.
	*Do not mix text and graphics-mode printing on the same page.
	*Only the following commands are available in graphics mode: 
		LF              Line feed
		FF              Form feed
		CR              Carriage return
		ESC+EM          Control paper loading/ejecting
		ESC+.           Print raster graphics
		ESC+@           Initialize printer (exit graphics mode)
		ESC+(+c         Set page format
		ESC+(+C         Set page length in defined unit
		ESC+(+V         Set absolute vertical print position
		ESC+(+v         Set relative vertical print position
		ESC+\           Set relative vertical print position
		ESC+$           Set absolute horizontal print position
		ESC+r           Select printing color
		ESC+U           Turn unidirectional mode on/off
		ESC++           Set n/360-inch line spacing
		ESC+(+U         Set unit
	 The printer ignores all other commands.

<RASTER GRAPHIC>
Print raster graphics

	SET :
	NAME:   ESC    .     c    v    h    m    n1    n2    Data
	Hex.:   1B     2E    c    v    h    m    n1    n2    Data
	Dec.:   27     46    c    v    h    m    n1    n2    Data

	Comment:
	*Parameter range:
		c = 0,1   
		v = 10,20 
		h = 10,20 
		0<=m<=24
		0<=n1<=255
		0<=n2<=127

	Notes:
	*Parameters are used as described below:
		c=0 non compressed graphics mode
		c=1 compressed graphics mode (Run-Length data compression).  
		    Data is treated as counter byte, data, counter byte, 
		    data, etc.
		    if c<128 
			counter byte = number of data bytes to follow - 1
		    if c>127
			counter byte = number of times to repeat the next
			byte of data calculated as follows: 
				257-counter byte
		v=vertical dot density (v/3600)
		h=horizontal dot density (h/3600)
		m=vertical dot count (rows of dot graphics)
		n1 and n2 = horizontal dot count (columns of dot graphics)
		   horizontal dot count = n1 + (n2 x 256)
	*This command can be used only during graphics mode, entered by 
	 sending the ESC+(+G command.
	*The combination of v = 10 and h = 20 (360 vertical dots by 180 
	 horizontal dots) is not possible.
	*You can specify the horizontal dot count in 1-dot increments. If the
	 dot count is not a multiple of 8, the remaining data in the data byte 
	 at the far right of each row is ignored.
	*The final print position is the dot after the far right dot on the 
	 top row of the graphics printed with this command.
	*Repetitive data bytes can be mixed with data blocks in the same 
	 command.
	*You cannot move the print position in a negative direction (up)
	 immediately after this command. Also, the printer ignores commands
	 moving the vertical print position in a negative direction if the 
	 final position would be above any graphics printed with this command.

<1/8 INCH PAPER FEED>
Sets paper feed amount to 1/8 inch (3.2 mm).

	Name:   ESC     0
	Dec.:   27      48
	Hex.:   1B      30

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<1/6 INCH PAPER FEED>
Sets paper feed amount to 1/6 inch (4.23 mm).

	Name:   ESC     2
	Dec.:   27      50
	Hex.:   1B      32

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<n/60 INCH PAPER FEED>
Sets paper feed amount to n/60 inch.

	Name:   ESC     A       n       (n = 0 to 127)DEC
	Dec.:   27      65      n
	Hex.:   1B      41      n

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<n/180 INCH PAPER FEED>
Sets programmable paper feed amount to n/180 inch.

	Name:   ESC     3       n
	Dec.:   27      51      n
	Hex.:   1B      33      n

	Comments:
	*n/180 inch paper feed is valid for n = 0 to 255.
	*PANEL LOCK in the Function mode affects this command.

<n/360 INCH PAPER FEED>
Sets paper feed amount to n/360 inch.

	Name:   ESC     +       n       (n = 0 to 255)DEC
	Dec.:   27      43      n
	Hex.:   1B      2B      n

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<LINE FEED (LF)>
Feeds paper to next line position after printing data in the line buffer.

	Name:   LF
	Dec.:   10
	Hex.:   0A

	Comments:
	*The amount of spacing generated by LF is determined by the
	 paper feed commands or the Function mode setting.
	*When the new line position falls within the perforation skip
	 area, the paper advances to the next top of form position.

<FORM FEED (FF)>
Feeds paper to next top of form position after printing data 
in the line buffer.

	Name:   FF
	Dec.:   12
	Hex.:   0C

	Comment:
	*The amount of spacing generated by FF is determined
	 by the page length commands or the Function mode setting.

<n/180 INCH SINGLE LINE FEED>
Feeds paper n/180 inch after printing data in the line buffer.

	Name:   ESC     J       n       (n = 0 to 255)DEC
	Dec.:   27      74      n
	Hex.:   1B      4A      n

<n/180 INCH REVERSE DIRECTION SINGLE LINE FEED>
Prints data in the line buffer and feeds the paper n/180 inch 
in the reverse direction.

	Name:   ESC     j       n       (n = 0 to 255)DEC
	Dec.:   27      106     n
	Hex.:   1B      6A      n

	Note:
	*Reverse paper feed cannot be executed in the area within
	 3.6inches (91.4 mm) of the bottom perforation. Additionally,
	 the perforation should not be included in the area of
	 reverse paper feed.
	*In the pull tractor mode, this command will not reverse feed
	 paper correctly and resulting printout may not be correct.

<PAGE LENGTH (INCHES)>
Sets page length in inches.

	Name:   ESC     C       0       n       (n = 0 to 22)DEC
	Dec.:   27      67      0       n
	Hex.:   1B      43      00      n

	Comments:
	*Upon receipt of ESC+C+0+n, the present line position becomes
	 the top of form position.
	*ESC+C+0+n releases the skip perforation settings.
	*The page length does not change even if the paper feed amount
	 is changed.
	*The terms "form" and "page" are interchangeable.
	*PANEL LOCK in the Function mode affects this command.

<PAGE LENGTH (LINES)>
Sets page length in number of lines.

	Name:   ESC     C       n       (n = 1 to 127)DEC
	Dec.:   27      67      n
	Hex.:   1B      43      n

	Comments:
	*Upon receipt of ESC+C+n, the present line position becomes
	 the top of form position.
	*If n=0, page length returns to the inch designation.
	*ESC+C+n releases the skip perforation settings.
	*The page length does not change even if the paper feed amount
	 is changed
	*The terms "form" and "page" are interchangeable.
	*PANEL LOCK in the Function mode affects this command.

<LEFT MARGIN>
Sets position of left margin.

	Name:   ESC     l       n
	Dec.:   27      108     n
	Hex.:   1B      6C      n

	Comments:
	*The following values of n can be used:
					8" print line	  9" print line
		-------------------------------------------------------
		Pica print              n = 0 to 78       n=0 to 88
		Elite print             n = 0 to 93       n=0 TO 105
		Micron print            n = 0 to 117      n=0 to 133
		Compressed print        n = 0 to 133      n=0 to 151
		
	*If the value of n exceeds the right margin value, ESC+l+n
	 is ignored.
	*Setting the left margin clears all data in the line buffer.
	*In proportional spacing, the value of n is based on 10 CPI.
	*Once the left margin position is set, a change in the
	 character mode will not alter this left margin setting.
	*PANEL LOCK in the Function mode affects this command.

<RIGHT MARGIN>
Sets position of right margin.

	Name:   ESC     Q       n
	Dec.:   27      81      n
	Hex.:   1B      51      n

	Comments:
	The following values of n can be used:
					8" print line	  9" print line
		-------------------------------------------------------
		Pica print              n = 2 to 80       n=2 to 90
		Elite print             n = 3 to 96       n=3 TO 108
		Micron print            n = 3 to 120      n=3 to 136
		Compressed print        n = 4 to 137      n=4 to 155

	*If the value n exceeds the left margin value, ESC+Q+n is
	 ignored.
	*Setting the right margin clears all data in the line buffer.
	*In proportional spacing, the value of n is based on 10 CPI.
	*Once the right margin position is set, a change in the
	 character mode will not alter this right margin setting.
	*PANEL LOCK in the Function mode affects this command.

<SKIP PERFORATION>
Sets skip perforation.

	Set:
	Name:   ESC     N       n        (n = 1 to 127)DEC
	Dec.:   27      78      n
	Hex.:   1B      4E      n

	Release:
	Name:   ESC     O
	Dec.:   27      79
	Hex.:   1B      4F

	Comments:
	*The value of n specifies the number of lines (or n times the current
	 line spacing amount) to be skipped at the bottom of the page.
	*If n>128, the value is processed as n-128. If n=128 the command
	 is ignored.
	*The skip perforation amount does not change even if the paper feed
	 amount is changed following a skip perforation designation.
	*The skip perforation setting is released upon receipt of the page
	 length designation command.
	*The skip perforation command overrides the front panel Bottom 
	 margin setting. 
	*PANEL LOCK in the Function mode affects this command.

<PAGE LENGTH (UNIT)>
Set page length in defined unit

	SET :
	NAME:   ESC     (       C       2       0       n1      n2
	Hex.:   1B      28      43      2       0       n1      n2
	Dec.:   27      40      67      02      00      n1      n2

	Comment:
	*Parameter range:
		0<((n2 x 256)+n1) x (defined unit) <= 22

	Notes:
	*Define unit with the ESC ( U command. Default value = 1/360 inches.
	*Set the page length before paper is loaded or when the print position
	 is at the top-of-form position. Otherwise, the current print position
	 becomes the top-of-form position (this results in undesirable 
	 contradictions between the actual and logical page settings).
	*Setting the page length cancels the top and bottom-margin settings.
	*Changing the defined unit does not affect the current page-length
	 setting.


<PAGE FORMAT>   
Set page format

	SET :
	NAME:   ESC     (       c       4       0       m1      m2      n1   n2
	Hex.:   1B      28      63      4       0       m1      m2      n1   n2
	Dec.:   27      40      99      04      00      m1      m2      n1   n2

	Comments:
	*Top Margin = m1+(m2x256) x (defined unit) where top margin < bottom
	 margin.
	*Bottom Margin = n1+(n2x256) x (defined unit) where bottom margin <
	 22 inches.
	*Define unit with the ESC ( U command. Default value = 1/360 inches.
	*Measure both top and bottom margins from the top edge of the page.
	*The baseline for printing characters on the first line is 20/180 inch
	 below the top-margin position.
	*Send this command before paper is loaded, or when paper is at the top-
	 of-form position.  Otherwise, the current print position becomes the
	 top-margin position (this results in undesirable contradictions 
	 between the actual and logical page settings).
	*This command cancels any previous top and bottom-margin settings.
	*Changing the defined unit does not affect the current page-length 
	 setting.


<HORIZONTAL TAB STOP SETTING>
Sets horizontal tabulations to specified values.

	Set:
	Name:   ESC     D       n1      n2...nx         0
	Dec.:   27      68      n1      n2...nx         0
	Hex.:   1B      44      n1      n2...nx         00

	Release:
	Name:   ESC     D       0
	Dec.:   27      68      0
	Hex.:   1B      44      00

	Comments:
	*Horizontal tabs are set from the left margin position.
	*Horizontal tabs must be designated such that n1<n<2<...<nx.
	*A maximum of 32 tabs may be set on a single line.
	*ESC+D+n1+n2+...+nx+0 sets horizontal tab stops. The HT command
	 executes the tab designation.
	*In proportional spacing, horizontal tabs are set based on 10 CPI.
	*When the left margin is changed, horizontal tabs will be moved
	 based on new margin setting.
	*When the printer is powered up, tabs are automatically set every
	 8 characters.
	*If the pitch is altered after designation of horizontal tabs,
	 the tab positions do not move.

<HORIZONTAL TAB EXECUTION>
Executes the horizontal TAB as designated by ESC+D+n1+n2...+nx+0.

	Name:   HT
	Dec.:   9
	Hex.:   09

	Comments:
	*If the value of horizontal TAB is less than present column
	 position, then HT is ignored.
	*When in underline mode, the blank spaces between consecutive
	 HT print positions are not underlined.

<VERTICAL TAB STOP SETTING>
Sets vertical tabulation to specified values.

	Set:
	Name:   ESC     B       n1      n2...nx         0
	Dec.:   27      66      n1      n2...nx         0
	Hex.:   1B      42      n1      n2...nx         00

	Release:
	Name:   ESC     B       0
	Dec.:   27      66      0
	Hex.:   1B      42      00

	Comments:
	*VT is set from the top of form position.
	*Vertical tabs must be designed such that n1<n2...<nx.
	*ESC+B+n1+n2+...+nx+0 sets vertical tab stops. The VT
	 command executes the tab designation.
	*If the paper feed amount is changed after a designation
	 of vertical tabs, the positions do not change.
	*VT settings are released by page length designation commands.
	*A maximum of 16 tabs may be set.

<VERTICAL TAB EXECUTION>
Executes the vertical TAB as designated by
ESC+B+n1+n2+...+nx+0, ESC+b+m+n1+n2+...nx+0.

	Name:   VT
	Dec.:   11
	Hex.:   0B

	Comments:
	*When TABs are set with VT or VFU setting command and when
	 there is no tab setting on a position exceeding the present
	 line, data in the line buffer is printed and the paper is fed
	 to the next top of form position (same as FF).
	*On power up no vertical tabs have been set; therefore, when
	 a VT is sent, the paper advances one line.
	*When vertical TAB is cleared by ESC+B+0, execution of VT
	 causes data in the line buffer to be printed and does not
	 advance the paper.

<BACKSPACE>
Prints data in the line buffer and backspaces one space.

	Name:   BS
	Dec.:   8
	Hex.:   08

	Comment:
	*The backspacing amount will depend upon the pitch set when
	 the BS code is executed.

<CARRIAGE RETURN>
Prints data in the line buffer and returns the printhead
to the left margin position.

	Name:   CR
	Dec.:   13
	Hex.:   0D

	Comments:
	*Certain computers issue an automatic line feed with
	 a carriage return. Check your computer manual for details.
	*When automatic LF is set to ON through the initial setup mode
	 or through initial setup disk, a LF is executed whenever a CR
	 code is executed.


<ONE LINE UNI-DIRECTION>
Causes printhead to move to its left margin position.

	Name:   ESC     <
	Dec.:   27      60
	Hex.:   1B      3C


<UNI-DIRECTION>
Sets uni-directional printing mode.

	Set:
	Name:   ESC     U       1
	Dec.:   27      85      1
	Hex.:   1B      55      01

	Release:
	Name:   ESC     U       0
	Dec.:   27      85      0
	Hex.:   1B      55      00

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<HALF SPEED PRINTING>
Sets printing to half speed.

	Set:
	Name:   ESC     s       1
	Dec.:   27      115     1
	Hex.:   1B      73      01

	Release:
	Name:   ESC     s       0
	Dec.:   27      115     0
	Hex.:   1B      73      00

	Comment:
	*Half speed printing can be set only in the draft pica,
	 draft elite, standard density image, double-speed
	 double-density image, CRT I image and CRT II image modes.

<ABSOLUTE HORIZONTAL POSITION>
Moves the printhead to an absolute horizontal position.

	Name:   ESC     $       n1      n2
	Dec.:   27      36      n1      n2
	Hex.:   1B      24      n1      n2

	Comments:
	*This command moves the print position to a position
	 n1+256xn2 dots (units) from the left margin. Each unit
	 equals 1/60th of an inch.
	*To calculate n1 and n2 first determine the total increments
	 of 1/60 inch to move the print position from the left margin.
	 Let this value = m then
		n1=m MOD 256
		n2=int(m/256)

<RELATIVE HORIZONTAL POSITION>
Moves the printhead left or right to a relative horizontal position.

	Name:   ESC     \       n1      n2
	Dec.:   27      92      n1      n2
	Hex.:   1B      5C      n1      n2

	Comments:
	*This command moves the print position n/120 (in draft mode) or 
	 n/180 (in LQ mode) of an inch from current position.
	*To calculate n1 and n2 first determine the total increments of
	 1/120 (in draft mode) or n/180 (in LQ mode) of an inch to move 
	 the print position from its current position.
	*If the head movement will be to the left subtract this number
	 from 65536.
	*To move n/120 (draft) or n/180 (LQ) of an inch to right: m=n
	 To move n/120 (draft) or n/180 (LQ) of an inch to left: m=65536-n
		 n1=m MOD 256   n2=int(m/256)
	*If the resulting movement would place the printhead outside
	 current margins, the command is ignored.

<ABSOLUTE VERTICAL POSITION>
Set absolute vertical print position

	SET :
	NAME:   ESC     (       V       2       0       n1      n2
	Hex.:   1B      28      56      2       0       n1      n2
	Dec.:   27      40      86      02      00      n1      n2

	Comment:
	*Parameter range:
		0<=n1<=255
		0<=n2<=127

	Notes:
	*Set the defined unit using the ESC+(+U command.
	*The default defined unit for this command is 1/360 inch.
	*The new position is (n1+(n2x256)) x (defined unit) inches from 
	 the current top margin position.
	*Moving the print position below the bottom-margin position produces
	 the following results:
	 Continuous paper       Moves the vertical print position to the 
				top-margin position on the next page
	 Single-sheet paper     Ejects the paper
	*The printer ignores this command under the following conditions:
	 - The command would move the print position more than 1/2 inch in the
	   negative direction
	 - The command would move the print position in the negative direction
	   after a graphics command is sent on the current line

<RELATIVE VERTICAL POSITION>
Set relative vertical print position

	SET :
	NAME:   ESC     (       v       2       0       n1      n2
	Hex.:   1B      28      76      2       0       n1      n2
	Dec.:   27      40      118     02      00      n1      n2

	Comment:
	*Parameter range:
		0<=n1<=255		For positive movement:
		0<=n2<=127		    0<=n2<=63
					For negative movement:
					    64<=n2<=127

	Notes:
	*Set the defined unit using the ESC+(+U command.
	*The default defined unit for this command is 1/360 inch.
	*The new position is (n1+(n2x256)) x (defined unit) from the 
	 current vertical position.
	*Moving the print position below the bottom-margin position produces 
	 the following results:
	 Continuous paper       Moves the vertical print position to the 
				top-margin position on the next page
	 Single-sheet paper     Ejects the paper
	*The printer ignores this command under the following condition:
	 - The command would move the print position in the negative direction
	   after a graphics command is sent on the current line.

<CANCEL>
Clears all data in the line buffer.

	Name:   CAN
	Dec.:   24
	Hex.:   18

<REMOTE PRINTER SELECT>
Selects printer after it has been deselected by DC3.

	Name:   DC1     (Device Control 1)
	Dec.:   17
	Hex.:   11

	Comment:
	*All data sent to the printer between DC3 and DC1 is lost.

<REMOTE PRINTER DESELECT>
Deselects printer until it has been selected by DC1.

	Name:   DC3     (Device Control 3)
	Dec.:   19
	Hex.:   13

	Comment:
	*All data sent to the printer between DC3 and DC1 is lost.

<DELETE>
Deletes the last character stored in the line buffer.

	Name:   DEL
	Dec.:   127
	Hex.:   7F

	Comment:
	*Only text characters may be deleted. Bit image data, spacing
	 generated by consecutive TABs, and commands cannot be deleted.

<MSB ON>
Sets the Most Significant Bit to 1.

	Name:   ESC     >
	Dec.:   27      62
	Hex.:   1B      3E

	Comments:
	*ESC+> has no effect on bit image data.
	*This setting can be released by ESC+#.
	*PANEL LOCK in the Function mode affects this command.

<MSB OFF>
Sets the Most Significant Bit to 0.

	Name:   ESC     =
	Dec.:   27      61
	Hex.:   1B      3D

	Comments:
	*ESC+"=" has no effect on bit image data.
	*This setting can be released by ESC+#.
	*PANEL LOCK in the Function mode affects this command.

<CANCELS MSB SETTING>
Sets printer to receive 8th bit as is.

	Name:   ESC     #
	Dec.:   27      35
	Hex.:   1B      23

	Comments:
	*This setting has no effect on bit image data.
	*PANEL LOCK in the Function mode affects this command.

<FONT DOWNLOADING>
Defines download characters into specified address locations in RAM.

	Name:   ESC  &    0    n    m    d0   d1   d2   Data
	Dec.:   27   38   0    n    m    d0   d1   d2   Data
	Hex.:   1B   26   00   n    m    d0   d1   d2   Data

	Comments:
	*The values n and m are the ASCII address locations of the
	 first and last characters being defined.
	*The values of d0, d1 and d2 define the character cell.
	*d0=Left Space d1=Body d2=Right Space
	*The values of d0,d1 and d2 vary with pitch as follows:

			d1       d0+d1+d2 (total)
	Draft           9               12
	LQ 10 CPI       29              36
	LQ 12 CPI       23              30
	LQ 15 CPI       15              24
	PS              37              42

	*PANEL LOCK in the Function mode affects this command.
	*This command is operational only when DOWNLOAD is set to ON
	 through the Function mode or setup disk.
	*Draft and Letter Quality (LQ) fonts can be downloaded simultaneously. 
	 Draft download characters are printed when the printer is 
	 in draft mode. LQ characters are printed when the printer is 
	 in LQ mode.
	*Making Maximum Use of the Buffer:
	 Epson mode:
	 18K (18,432) bytes are available and can be divided between draft
	 and LQ characters in any combination, subject to hexadecimal
	 address and buffer limits. Draft letters require 39 bytes maximum
	 and LQ letters require 114 maximum. To determine if the desired
	 combination will fit, use the formula:

	 (# of draft characters x 39)+(# of LQ characters x 114) <= 18,432

	 For example:
	 120 draft and 120 LQ are desired.
	 (120 x 39)+(120 x 114) = 4,680+13,680 = 18,360
	 Therefore this combination will fit.

	 Because no more than 256 addresses can be identified in 1 byte
	 (00h-FFh), 256 is the maximum number of draft characters that can
	 be defined. The maximum number of LQ characters that can be loaded
	 is 161.

	*Designing Download Characters

	 1. Draft Font
	 To download a character you must first design the character.
	 A draft font download character uses 9 columns and 24 rows of
	 dots. Since a given column contains 24 dots, each column is divided
	 into 3 portions, upper 8, middle 8 and lower 8 dots. Column 1 is
	 labeled P1H for the upper 8 dots, P1M for the middle 8 and P1L for
	 the lower 8 dots. Similarly, column 9 is labeled P9H for the upper
	 8 dots, P9M for the middle 8 and P9L for the lower 8 dots. Column
	 10, 11 and 12 are always set to zero, thus we are working with P1H
	 through P9L.
	 In the matrix below, the circles represent pins that may be fired.
	 You may darken any circle, provided no two adjacent horizontal
	 circles are filled in. Once you have designed the character, you
	 must quantify each dot column, P1H-P9H, by summing the powers of
	 two represented by each dot. Consider the design of the Greek
	 character gamma.

					 Character body   Right space columns
		_____________            <---------------><---->
			     2^7 (128)   . . . . . . . . . . . .
			     2^6 (64)    . . . . . . . . . . . .
			     2^5 (32)    . . . . . . . . . . . .
		Upper        2^4 (16)    . . . . . . . . . . . .
		  8 dots (H) 2^3 (8)     . . . . . . . . . . . .
			     2^2 (4)     . . . . . . . . . . . .
			     2^1 (2)     . . . . . . . . . . . .
		_____________2^0 (1)     . . O . . . . . O . . .
			     2^7 (128)   . O . O . . . . . . . .
			     2^6 (64)    . . . . O . . . O . . .
			     2^5 (32)    . . . . . . . . . . . .
		Middle       2^4 (16)    . . . . . O . O . . . .
		  8 dots (M) 2^3 (8)     . . . . . . . . . . . .
			     2^2 (4)     . . . . . . O . . . . .
			     2^1 (2)     . . . . . O . . . . . .
		_____________2^0 (1)     . . . . O . O . . . . .
			     2^7 (128)   . . . . . . . . . . . .
			     2^6 (64)    . . . . O . O . . . . .
			     2^5 (32)    . . . . . . . . . . . .
		Lower        2^4 (16)    . . . . . O . . . . . .
		  8 dots (L) 2^3 (8)     . . . . . . . . . . . .
			     2^2 (4)     . . . . . . . . . . . .
			     2^1 (2)     . . . . . . . . . . . .
		_____________2^0 (1)     . . . . . . . . . . . .

					 : : : : : : : : :
	P1H=0, P1M=0,   P1L=0  ..........: : : : : : : : :
					   : : : : : : : :
	P2H=0, P2M=128, P2L=0  ............: : : : : : : :
					     : : : : : : :
	P3H=1, P3M=0,   P3L=0  ..............: : : : : : :
					       : : : : : :
	P4H=0, P4M=128, P4L=0  ................: : : : : :
						 : : : : :
	P5H=0, P5M=65,  P5L=64 ..................: : : : :
						   : : : :
	P6H=0, P6M=18,  P6L=16 ....................: : : :
						     : : :
	P7H=0, P7M=5,   P7L=64 ......................: : :
						       : :
	P8H=0, P8M=16,  P8L=0  ........................: :
							 :
	P9H=1, P9M=64,  P9L=0  ..........................:

	 2. LQ Font
	 A LQ font download character uses 36 columns and 24 rows of dots.
	 Designing and storing fonts can be performed in the same way as
	 with draft fonts. Here, consider the design of the one-eighth-note
	 character:

				      Left space  Character body  Right space
		_____________            <----><------------------><-------->
			     2^7 (128)   ....................................
			     2^6 (64)    ....................................
			     2^5 (32)    ................O...................
		Upper        2^4 (16)    ................O...................
		  8 dots (H) 2^3 (8)     ................O.O.................
			     2^2 (4)     ................O.O.O...............
			     2^1 (2)     ................O.O.O.O.............
		_____________2^0 (1)     ................O.....O.O...........
			     2^7 (128)   ................O.......O...........
			     2^6 (64)    ................O........O..........
			     2^5 (32)    ................O........O..........
		Middle       2^4 (16)    ................O........O..........
		  8 dots (M) 2^3 (8)     ................O........O..........
			     2^2 (4)     ..........O.O...O.......O...........
			     2^1 (2)     ........O.O.O.O.O...................
		_____________2^0 (1)     .......O.O.O.O.O....................
			     2^7 (128)   ......O.O.O.O.O.O...................
			     2^6 (64)    .......O.O.O.O.O....................
			     2^5 (32)    ........O.O.O.O.....................
		Lower        2^4 (16)    ..........O.O.......................
		  8 dots (L) 2^3 (8)     ....................................
			     2^2 (4)     ....................................
			     2^1 (2)     ....................................
		_____________2^0 (1)     ....................................

					       ::::::::::::::::::::
	P7H=0,   P7M=0,    P7L=128  ...........::::::::::::::::::::
						:::::::::::::::::::
	P8H=0,   P8M=1,    P8L=64   ............:::::::::::::::::::
						 ::::::::::::::::::
	P9H=0,   P9M=2,    P9L=160  .............::::::::::::::::::
						  :::::::::::::::::
	P10H=0,  P10M=1,   P10L=64  ..............:::::::::::::::::
						   ::::::::::::::::
	P11H=0,  P11M=6,   P11L=176 ...............::::::::::::::::
						    :::::::::::::::
	P12H=0,  P12M=1,   P12L=64  ................:::::::::::::::
						     ::::::::::::::
	P13H=0,  P13M=6,   P13L=176   ...............::::::::::::::
						      :::::::::::::
	P14H=0,  P14M=1,   P14L=64   .................:::::::::::::
						       ::::::::::::
	P15H=0,  P15M=2,   P15L=160  ..................::::::::::::
							:::::::::::
	P16H=0,  P16M=1,   P16L=64   ...................:::::::::::
							 ::::::::::
	P17H=63, P17M=254, P17L=128  ....................::::::::::
							  :::::::::
	P18H=0,  P18M=0,   P18L=0   ......................:::::::::
							   ::::::::
	P19H=14, P19M=0,   P19L=0   .......................::::::::
							    :::::::
	P20H=0,  P20M=0,   P20L=0  .........................:::::::
							     ::::::
	P21H=6,  P21M=0,   P21L=0   .........................::::::
							      :::::
	P22H=0,  P22M=0,   P22L=0  ...........................:::::
							       ::::
	P23H=3,  P23M=0,   P23L=0   ...........................::::
								:::
	P24H=0,  P24M=0,   P24L=0   ............................:::
								 ::
	P25H=1,  P25M=132, P25L=0   .............................::
								  :
	P26H=0,  P26M=120, P26L=0   ..............................:


	*Entering Download Data
	 Epson mode:

	 1. Draft Font
	 Download command in the Epson mode is:
		ESC+"&"+0+n+m+d0+d1+d2+DATA

	 Input format for a download command is:
		LPRINT CHR$(27)+"&"+CHR$(0)+CHR$(n)+CHR$(m)+
				    CHR$(d0)+CHR$(d1)+CHR$(d2)+DATA

	 Programming example for the Greek character gamma is as follows:

	 10 REM Draft Download Character
	 20 WIDTH "LPT1:",255
	 30 OPEN "LPT1:" AS #1
	 40 PRINT #1,CHR$(27)+"x0";
	 50 PRINT #1,CHR$(27)+":"+CHR$(0)+CHR$(0)+CHR$(0);
	 60 PRINT #1,CHR$(27)+"&"+CHR$(0)+CHR$(65)+CHR$(65);
	 70 PRINT #1,CHR$(1)+CHR$(8)+CHR$(3);
	 80 PRINT #1,CHR$(0)+CHR$(128)+CHR$(0);
	 90 PRINT #1,CHR$(1)+CHR$(0)+CHR$(0);
	 100 PRINT #1,CHR$(0)+CHR$(128)+CHR$(0);
	 110 PRINT #1,CHR$(0)+CHR$(65)+CHR$(64);
	 120 PRINT #1,CHR$(0)+CHR$(18)+CHR$(16);
	 130 PRINT #1,CHR$(0)+CHR$(5)+CHR$(64);
	 140 PRINT #1,CHR$(0)+CHR$(16)+CHR$(0);
	 150 PRINT #1,CHR$(1)+CHR$(64)+CHR$(0);
	 160 REM Download Character Print
	 170 PRINT #1,CHR$(27)+"%"+CHR$(1);
	 180 PRINT #1,"A A A A A A A A A A";CHR$(10);
	 190 PRINT #1,CHR$(27)+"%"+CHR$(0);
	 200 END

	 First determine where in RAM the character(s) should be stored.
	 The variables "n" and "m" are used for this purpose. The value
	 specified for n indicates the location into which the first
	 download character will be stored. The value specified for "m"
	 indicates the location into which the last download character will
	 be stored. If you are storing a single character, then n=m.

	 Next define the value of "d0", "d1" and "d2", which specify
	 attribute information. The attribute information includes the
	 following:

	 d0=number of space dot columns to the left of the character body
	 d1=number of character body dot columns
	 d2=number of space dot columns to the right of the character body

	 In our sample program, we created a gamma character. This character
	 consists of 1 left space dot column, 8 body dot columns and 3 right
	 space dot columns. Therefore, d0=1, d1=8 and d2=3.
	 In general, d1 cannot exceed 9 and d0+d1+d2 cannot exceed 12.

	 Note:
	 Program line 40 is necessary for downloading the draft font and
	 designates draft printing.
	 Program lines 80-150 use the eight values P2H-P9L to define the
	 shape and size of the gamma.
	 Program line 170 selects download character generator. After this
	 selection, by printing the download code [in this example,
	 CHR$(65)="A"] the downloaded character is printed.
	 Two horizontal adjacent columns cannot be printed in either draft
	 or LQ mode.

	 2. LQ Font

	 Input format is the same as with draft fonts.
	 Programming example for the one-eighth-note character is as follows:

	 10 REM Define Download Letter Quality Character
	 20 WIDTH "LPT1:",255
	 30 OPEN "LPT1:" AS #1
	 40 PRINT #1,CHR$(27)+"x1";
	 50 PRINT #1,CHR$(27)+":"+CHR$(0)+CHR$(0)+CHR$(0);
	 60 PRINT #1,CHR$(27)+"&"+CHR$(0)+CHR$(65)+CHR$(65);
	 70 PRINT #1,CHR$(6)+CHR$(20)+CHR$(10);
	 80 PRINT #1,CHR$(0)+CHR$(0)+CHR$(128);
	 90 PRINT #1,CHR$(0)+CHR$(1)+CHR$(64);
	 100 PRINT #1,CHR$(0)+CHR$(2)+CHR$(160);
	 110 PRINT #1,CHR$(0)+CHR$(1)+CHR$(64);
	 120 PRINT #1,CHR$(0)+CHR$(6)+CHR$(176);
	 130 PRINT #1,CHR$(0)+CHR$(1)+CHR$(64);
	 140 PRINT #1,CHR$(0)+CHR$(6)+CHR$(176);
	 150 PRINT #1,CHR$(0)+CHR$(1)+CHR$(64);
	 160 PRINT #1,CHR$(0)+CHR$(2)+CHR$(160);
	 170 PRINT #1,CHR$(0)+CHR$(1)+CHR$(64);
	 180 PRINT #1,CHR$(63)+CHR$(254)+CHR$(128);
	 190 PRINT #1,CHR$(0)+CHR$(0)+CHR$(0);
	 200 PRINT #1,CHR$(14)+CHR$(0)+CHR$(0);
	 210 PRINT #1,CHR$(0)+CHR$(0)+CHR$(0);
	 220 PRINT #1,CHR$(6)+CHR$(0)+CHR$(0);
	 230 PRINT #1,CHR$(0)+CHR$(0)+CHR$(0);
	 240 PRINT #1,CHR$(3)+CHR$(0)+CHR$(0);
	 250 PRINT #1,CHR$(0)+CHR$(0)+CHR$(0);
	 260 PRINT #1,CHR$(1)+CHR$(132)+CHR$(0);
	 270 PRINT #1,CHR$(0)+CHR$(120)+CHR$(0);
	 280 REM Download Character Print
	 290 PRINT #1,CHR$(27)+"%"+CHR$(1);
	 300 PRINT #1,"A A A A A A A A A A";CHR$(10);
	 310 PRINT #1,CHR$(27)+"%"+CHR$(0);
	 320 END

	 The number of printable columns for characters downloaded in the
	 letter quality font is as follows:

				     d0+d1+d2
		LQ 10 CPI               36
		LQ 12 CPI               30
		Proportional Spacing    42

	*Print Mode Combination:
	 Draft Download characters can be printed only when the FONT is
	 set to Draft through software commands or the Function mode.
	 Letter quality download characters can be printed only when the
	 FONT is set to Bold PS, Courier, Orator, Prestige, Roman, Sans Serif,
	 Script or OCR-B through the Function mode or through software 
	 commands.

<SELECTS ROM CG OR DOWNLOADED CG>

	Name:   ESC     %       n
	Dec.:   27      37      n
	Hex.:   1B      25      n

	Comments:
	*The following values of n can be used.
		n=0: Select ROM Character Generator (CG)
		n=1: Select download CG
	*PANEL LOCK in the Function mode affects this command.

<ROM CHARACTER GENERATION SET COPY>
Copies both draft and LQ internal ROM CG font into the
downloadable font area.

	Name:   ESC     :       0       n       0       (n = 0 through 6)
	Dec.:   27      58      0       n       0
	Hex.:   1B      3A      00      n       00

	Comments:
	*The value of n specifies the LQ font to download.
	 Refer to Font Style command ESC+"k"+n.
	*Upon receipt of the command, all previous downloaded fonts
	 are cleared.
	*When altering only part of the ROM CG, use this command
	 before font downloading.
	*PANEL LOCK in the Function mode affects this command.

<BELL>
Sounds buzzer for approximately 0.5 second.

	Name:   BEL     
	Dec.:    7      
	Hex.:   07      

<RESET PRINTER>
Initializes printer, causing data in the line buffer,
but not in the receive buffer, to be cleared.

	Name:   ESC     @
	Dec.:   27      64
	Hex.:   1B      40

<SELECTS CSF>
Selects Cut Sheet Feeder (CSF) mode ON/OFF.

	Name:   ESC     EM      n
	Dec.:   27      25      n
	Hex.:   1B      19      n

	Comments:
	*The following values of n can be used.
		n=R: Eject a sheet
		n=0: Cut Sheet Feeder mode is OFF
		n=4: Cut Sheet Feeder mode is ON 
	*PANEL LOCK in the Function mode affects this command.

	Note:
	*If the Cut Sheet Feeder mode is set to ON without
	 installing the CSF, the paper will not feed correctly.

<PRINT COLOR>
Select printing color

	SET :
	NAME:   ESC    r     n    
	Hex.:   1B     72    n    
	Dec.:   27     114   n    

	Comment:
	*The following values of n can be used:
		n=0     Black
		n=1     Red (Magenta)
		n=2     Blue (Cyan)
		n=3     Violet
		n=4     Yellow
		n=5     Orange (Red)
		n=6     Green

	Notes:
	*This command is operational only when the color kit (KX-PCK11) is
	 installed.
	*Print yellow first when overlapping colors.

< Epson Mode Characters (USA Normal)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0   -   -  30  30  36  36  18  36  36  36  30  36  36  36  30  30

     1  1   -   -  18  30  36  36  30  36  36  42  18  36  36  36  30  30

     2  2   -   -  30  30  36  36  36  30  30  42  30  36  36  36  30  30

     3  3   -   -  30  30  36  36  30  30  30  30  30  36  36  36  30  30

     4  4   -   -  30  30  36  36  36  24  30  30  36  36  36  36  30  30

     5  5   -   -  36  30  36  42  30  36  30  30  36  36  36  36  30  30

     6  6   -   -  36  30  36  36  24  36  30  36  30  36  36  36  30  30

     7  7   -   -  18  30  36  42  36  42  30  36  30  36  36  36  30  30

     8  8   -   -  24  30  36  36  36  30  30  36  30  36  36  36  30  30

     9  9   -   -  24  30  24  36  18  36  30  36  30  36  36  36  30  30

    10  A   -   -  30  18  30  30  24  30  30  42  30  36  36  36  30  30

    11  B   -   -  30  18  36  24  36  24  18  30  30  36  36  36  36  30

    12  C   -   -  18  30  36  30  18  18  18  30  30  36  36  36  30  30

    13  D   -   -  30  30  42  24  42  24  18  36  30  36  36  36  30  30

    14  E   -   -  18  30  36  30  36  30  36  42  30  36  36  36  30  30

    15  F   -   -  30  30  36  30  30  30  36  30  30  36  36  36  30  30

	Sub/Superscript PS width is 2/3 of Normal PS.
	Compressed PS width is 1/2 of Normal PS.
						    Unit:1/360 inch (0.07 mm)

< Epson Mode Characters (Multilingual Normal)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0   -   -  30  30  36  36  18  36  36  36  30  36  36  36  36  30

     1  1   -   -  18  30  36  36  30  36  36  42  18  36  36  36  30  30

     2  2   -   -  30  30  36  36  36  30  30  42  30  36  36  36  36  30

     3  3   -   -  30  30  36  36  30  30  30  30  36  36  36  36  36  30

     4  4   -   -  30  30  36  36  36  24  30  30  36  36  36  36  30  30

     5  5   -   -  36  30  36  42  30  36  30  30  36  36  36  18  36  30

     6  6   -   -  36  30  36  36  24  36  30  36  30  36  30  24  30  30

     7  7   -   -  18  30  36  42  36  42  30  36  30  36  36  24  36  30

     8  8   -   -  24  30  36  36  36  30  30  36  30  36  36  24  36  30

     9  9   -   -  24  30  24  36  18  36  30  36  36  36  36  36  42  30

    10  A   -   -  30  18  30  30  24  30  30  42  30  36  36  42  42  30

    11  B   -   -  30  18  36  24  36  24  18  30  30  36  36  42  36  24

    12  C   -   -  18  30  36  30  18  18  18  30  30  36  36  36  36  24

    13  D   -   -  30  30  42  24  42  24  18  36  30  30  36  18  30  30

    14  E   -   -  18  30  36  30  36  30  36  30  30  36  36  24  18  30

    15  F   -   -  30  30  36  30  30  30  36  30  30  36  30  36  20  30

	Sub/Superscript PS width is 2/3 of Normal PS.
	Compressed PS width is 1/2 of Normal PS.
						    Unit:1/360 inch (0.07 mm)

< Epson Mode Characters (Portugal Normal)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0   -   -  30  30  36  36  18  36  36  36  30  36  36  36  30  30

     1  1   -   -  18  30  36  36  30  36  36  36  18  36  36  36  30  30

     2  2   -   -  30  30  36  36  36  30  30  36  30  36  36  36  30  30

     3  3   -   -  30  30  36  36  30  30  30  30  36  36  36  36  30  30

     4  4   -   -  30  30  36  36  36  24  30  30  36  36  36  36  36  30

     5  5   -   -  36  30  36  42  30  36  30  30  36  36  36  36  36  30

     6  6   -   -  36  30  36  36  24  36  36  42  30  36  36  36  30  30

     7  7   -   -  18  30  36  42  36  42  30  36  30  36  36  36  30  30

     8  8   -   -  24  30  36  36  36  30  30  24  30  36  36  36  30  30

     9  9   -   -  24  30  24  36  18  36  36  36  36  36  36  36  30  30

    10  A   -   -  30  18  30  30  24  30  30  42  30  36  36  36  30  30

    11  B   -   -  30  18  36  24  36  24  24  30  30  36  36  36  30  30

    12  C   -   -  18  30  36  30  18  18  36  30  30  36  36  36  30  30

    13  D   -   -  30  30  42  24  42  24  18  42  30  36  36  36  30  30

    14  E   -   -  18  30  36  30  36  30  36  42  30  36  36  36  30  30

    15  F   -   -  30  30  36  30  30  30  36  36  30  36  36  36  30  30

	Sub/Superscript PS width is 2/3 of Normal PS.
	Compressed PS width is 1/2 of Normal PS.
						    Unit:1/360 inch (0.07 mm)

< Epson Mode Characters (Canada-French Normal)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0   -   -  30  30  36  36  18  36  36  36  18  36  36  36  30  30

     1  1   -   -  18  30  36  36  30  36  36  36  18  36  36  36  30  30

     2  2   -   -  30  30  36  36  36  30  30  36  30  36  36  36  30  30

     3  3   -   -  30  30  36  36  30  30  36  30  36  36  36  36  30  30

     4  4   -   -  30  30  36  36  36  24  36  36  30  36  36  36  36  30

     5  5   -   -  36  30  36  42  30  36  30  24  30  36  36  36  36  30

     6  6   -   -  36  30  36  36  24  36  30  36  24  36  36  36  30  30

     7  7   -   -  18  30  36  42  36  42  30  36  30  36  36  36  30  30

     8  8   -   -  24  30  36  36  36  30  30  30  24  36  36  36  30  30

     9  9   -   -  24  30  24  36  18  36  30  36  30  36  36  36  30  30

    10  A   -   -  30  18  30  30  24  30  30  42  30  36  36  36  30  30

    11  B   -   -  30  18  36  24  36  24  18  30  30  36  36  36  30  30

    12  C   -   -  18  30  36  30  18  18  18  30  30  36  36  36  30  30

    13  D   -   -  30  30  42  24  42  24  30  42  30  36  36  36  30  30

    14  E   -   -  18  30  36  30  36  30  36  42  30  36  36  36  30  30

    15  F   -   -  30  30  36  30  30  30  30  30  30  36  36  36  30  30

	Sub/Superscript PS width is 2/3 of Normal PS.
	Compressed PS width is 1/2 of Normal PS.
						    Unit:1/360 inch (0.07 mm)

< Epson Mode Characters (Norway Normal)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0   -   -  30  30  36  36  18  36  36  36  30  36  36  36  30  30

     1  1   -   -  18  30  36  36  30  36  36  42  18  36  36  36  30  30

     2  2   -   -  30  30  36  36  36  30  30  42  30  36  36  36  30  30

     3  3   -   -  30  30  36  36  30  30  30  30  36  36  36  36  30  40

     4  4   -   -  30  30  36  36  36  24  30  30  36  36  36  36  36  30

     5  5   -   -  36  30  36  42  30  36  30  30  36  36  36  36  36  30

     6  6   -   -  36  30  36  36  24  36  30  36  30  36  36  36  30  30

     7  7   -   -  18  30  36  42  36  42  30  36  30  36  36  36  30  30

     8  8   -   -  24  30  36  36  36  30  30  36  30  36  36  36  30  30

     9  9   -   -  24  30  24  36  18  36  30  36  30  36  36  36  30  30

    10  A   -   -  30  18  30  30  24  30  30  42  30  36  36  36  30  30

    11  B   -   -  30  18  36  24  36  24  18  30  30  36  36  36  30  30

    12  C   -   -  18  30  36  30  18  18  18  30  30  36  36  36  30  30

    13  D   -   -  30  30  42  24  42  24  18  36  30  36  36  36  30  30

    14  E   -   -  18  30  36  30  36  30  36  42  30  36  36  36  30  30

    15  F   -   -  30  30  36  30  30  30  36  30  30  36  36  36  30  30

	Sub/Superscript PS width is 2/3 of Normal PS.
	Compressed PS width is 1/2 of Normal PS.
						    Unit:1/360 inch (0.07 mm)

< Epson Mode Characters (Turkey Normal)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0   -   -  30  30  36  36  18  36  36  36  30  36  36  36  30  30

     1  1   -   -  18  30  36  36  30  36  36  42  18  36  36  36  30  30

     2  2   -   -  30  30  36  36  36  30  30  42  30  36  36  36  30  30

     3  3   -   -  30  30  36  36  30  30  30  30  36  36  36  36  30  30

     4  4   -   -  30  30  36  36  36  24  30  30  36  36  36  36  36  30

     5  5   -   -  36  30  36  42  30  36  30  30  36  36  36  36  36  30

     6  6   -   -  36  30  36  36  24  36  30  36  36  36  36  36  30  30

     7  7   -   -  18  30  36  42  36  42  30  36  36  36  36  36  30  30

     8  8   -   -  24  30  36  36  36  30  30  24  30  36  36  36  30  30

     9  9   -   -  24  30  24  36  18  36  30  36  30  36  36  36  30  30

    10  A   -   -  30  18  30  30  24  30  30  42  30  36  36  36  30  30

    11  B   -   -  30  18  36  24  36  24  18  30  30  36  36  36  36  30

    12  C   -   -  18  30  36  30  18  18  18  30  30  36  36  36  30  30

    13  D   -   -  30  30  42  24  42  24  18  36  30  36  36  36  30  30

    14  E   -   -  18  30  36  30  36  30  36  36  30  36  36  36  30  30

    15  F   -   -  30  30  36  30  30  30  36  30  30  36  36  36  30  30


	Sub/Superscript PS width is 2/3 of Normal PS.
	Compressed PS width is 1/2 of Normal PS.
						      Unit:1/360 inch (0.07 mm)

;
;                    *******************************
;                    *****  IBM Mode Commands  *****
;                    *******************************


<PRINT QUALITY>

	Name:   ESC     I       n
	Dec.:   27      73      n
	Hex.:   1B      49      n

	Comments:
	*The following values of n can be used.
		n=0:    Internal Draft 10 CPI mode
		n=2:    Internal LQ 10 CPI mode
		n=3:    Internal Proportional LQ mode
		n=4:    Download Draft 10 CPI mode
		n=6:    Download LQ 10 CPI mode
		n=7:    Download Proportional LQ mode
		n=8:    Internal Draft 12 CPI mode
		n=10:   Internal LQ 12 CPI mode
		n=12:   Download Draft 12 CPI mode
		n=14:   Download LQ 12 CPI mode
		n=16:   Internal Draft 17 CPI mode
		n=18:   Internal LQ 17 CPI mode
		n=20:   Download Draft 17 CPI mode
		n=22:   Download LQ 17 CPI mode
	*PANEL LOCK in the Function mode affects this command.

<TYPEFACE>
Selects LQ Typeface.

	Name:   ESC     k       n
	Dec.:   27      107     n
	Hex.:   1B      6B      n

	Comments:
	*The following values can be used.
		n=0:    Roman 
		n=1:    Sans Serif 
		n=2:    Courier
		n=3:    Prestige 
		n=4:    Script
		n=5:    OCR-B 
		n=6:    Bold PS
		n=7:    Orator 
	*Typeface must be reselected after any pitch change.
	*IBM characters in locations from 0 to 31DEC (except 19,
	 20, 21DEC) from 00 to 1FHEX (except 13, 14, 15HEX) and
	 from 250 to 255DEC (from F0 to FFHEX) are printed in
	 Courier font, regardless of font selection.
	*PANEL LOCK in the Function mode affects this command.

<SUB/SUPERSCRIPT FONT>
Selects sub/superscript font with characters printed
in the lower/upper 2/3 area of the line.

	Set:
	Name:   ESC     S       n
	Dec.:   27      83      n
	Hex.:   1B      53      n

	Release:
	Name:   ESC     T
	Dec.:   27      84
	Hex.:   1B      54

	Comments:
	*The following values of n can be used:
		n=0: Superscript
		n=1: Subscript
	*Sub/superscript font is 2/3 normal character height.
	*Sub/superscript characters are normal width.

<ELITE PITCH>
Sets printing to 12 characters per inch.

	Set:
	Name:   ESC     :
	Dec.:   27      58
	Hex.:   1B      3A

	Release:
	Name:   DC2
	Dec.:   18
	Hex.:   12

	Comments:
	*When in Letter Quality mode, ESC + : selects
	 the Prestige Typeface (Refer to ESC+I+n).
	*PANEL LOCK in the Function mode affects this command.

<COMPRESSED PITCH>
Sets printing to 17 characters per inch.

	Set:
	Name:   SI      or      ESC     SI
	Dec.:   15      or      27      15
	Hex.:   0F      or      1B      0F

	Release:
	Name:   DC2
	Dec.:   18
	Hex.:   12

	Comments: 
	*When in Letter Quality mode, SI or ESC + SI selects
	 the Courier Typeface (Refer to ESC+I+n).
	*PANEL LOCK in the Function mode affects this command.

<PROPORTIONAL SPACING>
Sets proportional spacing between characters.

	Set:
	Name:   ESC     P       1
	Dec.:   27      80      1
	Hex.:   1B      50      01

	Release:
	Name:   ESC     P       0
	Dec.:   27      80      0
	Hex.:   1B      50      00

	Comments: 
	*When in Letter Quality mode, ESC + P + 1 selects
	 the Bold PS Typeface (Refer to ESC+I+n).
	*PANEL LOCK in the Function mode affects this command.

<EMPHASIZED PRINTING>
Sets printing to twice the original horizontal dot density.

	Set:
	Name:   ESC     E
	Dec.:   27      69
	Hex.:   1B      45

	Release:
	Name:   ESC     F
	Dec.:   27      70
	Hex.:   1B      46

	Comments: 
	*Emphasized characters are printed at half speed
	 (100 cps in draft pica pitch).
	*PANEL LOCK in the Function mode affects this command.

<DOUBLE STRIKE PRINTING>
Sets double strike character printing.

	Set:
	Name:   ESC     G
	Dec.:   27      71
	Hex.:   1B      47

	Release:
	Name:   ESC     H
	Dec.:   27      72
	Hex.:   1B      48

	Comments:
	*Double strike printing prints each line twice,
	 with the second line slightly below the first
	 to create a bold appearance.
	*PANEL LOCK in the Function mode affects this command.

<DOUBLE WIDE PRINTING SINGLE LINE>
Sets double wide expanded printing for one line only.

	Set:
	Name:   SO      or      ESC     SO
	Dec.:   14              27      14
	Hex.:   0E              1B      0E

	Release:
	Name:   DC4     or      ESC     W       0
	Dec.:   20              27      87      0
	Hex.:   14              1B      57      00

	Comments:
	*Single line double wide printing is released when:
	 - a LF,FF or VT is executed.
	 - a CR is executed.
	 - DC4 or ESC+W+0 is executed.
	*PANEL LOCK in the Function mode affects this command.

<DOUBLE WIDE PRINTING>
Sets double wide expanded printing.

	Set:
	Name:   ESC     W       1
	Dec.:   27      87      1
	Hex.:   1B      57      01

	Release:
	Name:   ESC     W       0
	Dec.:   27      87      0
	Hex.:   1B      57      00

	Comments:
	*DC4 will not release the double wide printing set by ESC+W+1.
	*PANEL LOCK in the Function mode affects this command.

<DOUBLE HIGH AND DOUBLE WIDE PRINTING>
Sets printing to double high, double wide or both at the same time.

	Name:   ESC  [   @   4   0   0   0   m3  m4
	Dec.:   27   91  64  4   0   0   0   m3  m4
	Hex.:   1B   5B  40  04  00  00  00  m3  m4

	Comments:
	*The value of m3 selects both the line feed and character
	 height as follows:

			Function
	m3      Line feed       Character height
	----------------------------------------
	0       Unchanged       Unchanged
	1       Unchanged       Single-line
	2       Unchanged       Double-high
	16      Single          Unchanged
	17      Single          Single-high
	18      Single          Double-high
	32      Double          Unchanged
	33      Double          Single-high
	34      Double          Double-high

	*The value of m4 selects the character width as follows:
		m4=0:           No change
		m4=1:           Single-width
		m4=2:           Double-width
	*PANEL LOCK in the Function mode affects this command.
	*In the pull tractor mode, this command will not reverse feed
	 paper correctly and the resulting printout may not be correct.

<UNDERLINING>
Sets continuous underlining of characters.

	Set:
	Name:   ESC     -       1
	Dec.:   27      45      1
	Hex.:   1B      2D      01

	Release:
	Name:   ESC     -       0
	Dec.:   27      45      0
	Hex.:   1B      2D      00

	Comments:
	*Bit image data, spaces set by the HT code and IBM Graphic
	 characters will not be underlined.
	*Pin No. 24 of the printhead is used for underlining.

<OVERLINING>
Sets continuous overlining of characters.

	Set:
	Name:   ESC     _       1
	Dec.:   27      95      1
	Hex.:   1B      5F      01

	Release:
	Name:   ESC     _       0
	Dec.:   27      95      0
	Hex.:   1B      5F      00

	Comments:
	*Bit image data, spaces set by the HT code, IBM graphic
	 characters will not be overlined.
	*Pin No. 1 of the printhead is used for overlining.

<IBM CHARACTER SET 1>
Selects IBM Character Set 1.

	Name:   ESC     7
	Dec.:   27      55
	Hex.:   1B      37

	Comments:
	*Refer to character set tables in appendix of the operating
	 instruction manual.
	*PANEL LOCK in the Function mode affects this command.

<IBM CHARACTER SET 2>
Selects IBM Character Set 2.

	Name:   ESC     6
	Dec.:   27      54
	Hex.:   1B      36

	Comments:
	*Refer to character set tables in appendix of the operating
	 instruction manual.
	*PANEL LOCK in the Function mode affects this command.

<SETS CODE PAGE>
Changes the current code page.

	Name:   ESC  [    T    4    0    0    0    n1   n2
	Dec.:   27   91   84   4    0    0    0    n1   n2
	Hex.:   1B   5B   54   04   00   00   00   n1   n2

	Comments:
	*The values of n1 and n2 select the code pages as follows:
		n1=00H and n2=00H:              Current
		n1=01H and n2=B5H:              USA
		n1=03H and n2=52H:              Multilingual
		n1=03H and n2=5CH:              Portugal
		n1=03H and n2=5FH:              Canada French
		n1=03H and n2=61H:              Norway
		n1=03H and n2=59H:              Turkey
		Except the above:               Downloaded font
	*PANEL LOCK in the Function mode affects this command.
	*Refer to character set tables in appendix of the operating
	 instruction manual.

<8-PIN STANDARD DENSITY GRAPHICS>
Sets standard density graphic mode [60 dots per inch].

	Name:   ESC     K       n1      n2      Data
	Dec.:   27      75      n1      n2      Data
	Hex.:   1B      4B      n1      n2      Data

	Comment:
	*Refer to "ESC+*+m+n1+n2" command in Epson mode.


<8-PIN DOUBLE DENSITY GRAPHICS>
Sets double density graphic mode [120 dots per inch].

	Name:   ESC     L       n1      n2      Data
	Dec.:   27      76      n1      n2      Data
	Hex.:   1B      4C      n1      n2      Data

	Comment:
	*Refer to "ESC+*+m+n1+n2" command in Epson mode.

<DOUBLE SPEED, DOUBLE DENSITY GRAPHICS>
Sets double speed, double density graphics mode [120 dots per inch].

	Name:   ESC     Y       n1      n2      Data
	Dec.:   27      89      n1      n2      Data
	Hex.:   1B      59      n1      n2      Data

	Comments:
	*Horizontal adjacent dots cannot be printed.
	*Refer to "ESC+*+m+n1+n2" command in Epson mode.

<8-PIN QUADRUPLE DENSITY GRAPHICS>
Sets quadruple density graphics mode [240 dots per inch].

	Name:   ESC     Z       n1      n2      Data
	Dec.:   27      90      n1      n2      Data
	Hex.:   1B      5A      n1      n2      Data

	Comments:
	*Horizontal adjacent dots cannot be printed.
	*Refer to "ESC+*+m+n1+n2" command in Epson mode.

<BIT IMAGE MODE SELECTION (AGM)>
Selects one of the 8-pin and 24-pin bit image graphic modes (AGM only).

	Name:   ESC     *       m       n1      n2      Data
	Dec.:   27      42      m       n1      n2      Data
	Hex.:   1B      2A      m       n1      n2      Data

	Comments:
	*The following table illustrates the various modes
	 based upon the values of m.

	m    pin  dpi   dpl
	----------------------------------------------------
	 0    8    60    540    Standard Density
	 1    8   120   1080    Double Density
	 2    8   120   1080    Double Speed, Double Density
	 3    8   240   2160    Quadruple Density
	 4    8    80    720    CRT I
	 6    8    90    810    CRT II
	32   24    60    540    Standard Density
	33   24   120   1080    Double Density
	38   24    90    810    CRT III
	39   24   180   1620    Triple Density
	40   24   360   3240    Hex Density

	*When m=2, 3, 40, horizontal adjacent dots cannot be printed.
	*The values n1 and n2 indicate the number of graphic columns
	 to be printed.
	*This command is effective only when AGM mode is set to ON
	 through the initial setup disk or the Function mode.
	*Refer to "ESC+*+m+n1+n2" command in Epson mode.

<BIT IMAGE MODE SELECTION>
Selects one of the 8-pin or 24-pin bit image graphic modes.

	Name:   ESC     [       g       n1      n2      m       Data
	Dec.:   27      91      103     n1      n2      m       Data
	Hex.:   1B      5B      67      n1      n2      m       Data

	Comments:
	*The following table illustrates the various modes
	 based upon the values of m.

	m    pin  dpi   dpl
	----------------------------------------------------
	 0    8    60    540    Standard Density
	 1    8   120   1080    Double Density
	 2    8   120   1080    Double Speed, Double Density
	 3    8   240   2160    Quadruple Density
	 8   24    60    540    Standard Density
	 9   24   120   1080    Double Density
	11   24   180   1620    Triple Density
	12   24   360   3240    Hex Density

	*When m=2, 3, 12, horizontal adjacent dots cannot be printed.
	*The values n1 and n2 indicate the number of graphic columns
	 to be printed.
	*Refer to "ESC+*+m+n1+n2" command in Epson mode.

<1/8 INCH PAPER FEED>
Sets paper feed amount to 1/8 inch (3.2 mm).

	Name:   ESC     0
	Dec.:   27      48
	Hex.:   1B      30

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<7/72 INCH PAPER FEED>
Sets paper feed amount to 7/72 inch (2.5 mm).

	Name:   ESC     1
	Dec.:   27      49
	Hex.:   1B      31

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<LINE SPACING>
Executes line spacing set by ESC+A+n.

	Name:   ESC     2
	Dec.:   27      50
	Hex.:   1B      32

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<n/72 INCH PAPER FEED SELECTION>
Sets paper feed amount to n/72 inch or n/60 inch (AGM).

	Name:   ESC     A       n       (n = 0 to 255)DEC
	Dec.:   27      65      n
	Hex.:   1B      41      n

	Comments:
	*ESC+2 must be input after ESC+A+n for n/72 inch paper feed
	 to become effective (when AGM is set to OFF only).
	*In the AGM mode, this command sets one line paper feed of
	 n/60 inch.
	*PANEL LOCK in the Function mode affects this command.

<n/216 INCH PAPER FEED>
Sets paper feed amount to n/216 inch or n/180 inch (AGM).

	Name:   ESC     3       n       (n = 0 to 255)DEC
	Dec.:   27      51      n
	Hex.:   1B      33      n

	Comments:
	*The paper feed amount is not exactly n/216 inch, for the
	 minimum unit is 1/360 inch.
	*In the AGM mode, this command sets one line paper feed of
	 n/180 inch.
	*PANEL LOCK in the Function mode affects this command.

<PAPER FEED BASE UNIT>
Selects base unit for ESC+3 and ESC+J.

	Name:   ESC   [     \     4    0    0    0    n    0
	Dec.:   27    91    92    4    0    0    0    n    0
	Hex.:   1B    5B    5C    04   00   00   00   n    00

	Comments:
	*The following values of n can be used:
		n=180           n/180 inch base unit
		n=216           1/216 inch base unit

<AUTOMATIC LINE FEED MODE>
Automatically executes a line feed following a carriage return.

	Set:
	Name:   ESC     5       1
	Dec.:   27      53      1
	Hex.:   1B      35      01

	Release:
	Name:   ESC     5       0
	Dec.:   27      53      0
	Hex.:   1B      35      00

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<LINE FEED (LF)>
Feeds paper to next line position after printing data in the line buffer.

	Name:   LF
	Dec.:   10
	Hex.:   0A

	Comments:
	*The amount of spacing generated by LF is determined
	 by the paper feed commands or Function mode setting.
	*When the new line position falls within the skip perforation
	 area, the paper advances to the next top of form position.
	*When Auto CR is set to ON through the initial setup disk or the 
	 Function mode,a Carriage Return command (CR) is added to each 
	 Line Feed (LF).

<FORM FEED (FF)>
Feeds paper to next top of form position after printing data in the line buffer.
	Name:   FF
	Dec.:   12
	Hex.:   0C

	Comment:
	*The amount of spacing generated by FF is determined
	 by the page length commands or Function mode setting.

<n/216 INCH SINGLE LINE FEED>
Feeds paper n/216 inch or n/180 inch (AGM) after printing data
in the line buffer.

	Name:   ESC     J       n       (n = 0 to 255)DEC
	Dec.:   27      74      n
	Hex.:   1B      4A      n

	Comments:
	*When Auto CR is set to ON through the initial setup disk
	 or the Function mode, a carriage return command (CR) is 
	 added to each line feed.
	*The paper feed amount is not exactly n/216 inch, for the
	 minimum unit is 1/360 inch.
	*In the AGM mode, this command sets one line paper feed of
	 n/180 inch.

<PAGE LENGTH (INCHES)>
Sets page length in inches.

	Name:   ESC     C       0       n       (n = 1 to 255)DEC
	Dec.:   27      67      0       n
	Hex.:   1B      43      00      n

	Comments:
	*Upon receipt of ESC+C+0+n, the present line position
	 becomes the top of form position.
	*ESC+C+0+n releases the skip perforation settings.
	*The page length does not change even if the paper feed
	 amount is changed.
	*The terms "form" and "page" are interchangeable.
	*PANEL LOCK in the Function mode affects this command.

<PAGE LENGTH (LINES)>
Sets page length in number of lines.

	Name:   ESC     C       n       (n = 1 to 255)DEC
	Dec.:   27      67      n
	Hex.:   1B      43      n

	Comments:
	*Upon receipt of ESC+C+n, the present line position
	 becomes the top of form position.
	*If n=0, page length returns to the inch designation.
	*ESC+C+n releases the skip perforation settings.
	*The page length does not change even if the paper feed
	 amount is changed.
	*The terms "form" and "page" are interchangeable.
	*PANEL LOCK in the Function mode affects this command.

<MARGIN SET>
Sets positions of left and right margins.

	Name:   ESC     X       n1      n2
	Dec.:   27      88      n1      n2
	Hex.:   1B      58      n1      n2

	Comments:
	*The following values of n1 (left) and n2 (right) can be used:
			  8" print line		     9" print line
	Pica         n1=1 to 78   n2=3 to 80    n1=1 to 88   n2=3 to 90
	Elite        n1=1 to 93   n2=4 to 96    n2=1 to 105  n2=4 to 108
	Compressed   n1=1 to 133  n2=5 to 137   n3=1 to 151  n2=5 to 155

	*To keep current left or right margin, set n1=0 or n2=0.
	*Any right margin designation to the left of the left margin
	 position is ignored.
	*Setting the margin clears all data in the line buffer.
	*Once the margin position is set, a change in the pitch will
	 not alter this margin setting.
	*PANEL LOCK in the Function mode affects this command.

<SKIP PERFORATION>
Sets skip perforation.

	Set:
	Name:   ESC     N       n       (n = 0 to 255)
	Dec.:   27      78      n
	Hex.:   1B      4E      n

	Release:
	Name:   ESC     O
	Dec.:   27      79
	Hex.:   1B      4F

	Comments:
	*The value of n specifies the number of lines (or n times
	 the current line spacing amount) to be skipped at the bottom
	 of the page. 
	*The skip perforation amount does not change even if the paper 
	 feed amount is changed following a skip perforation designation.
	*The skip perforation is released upon receipt of the page
	 length designation command.
	*The skip perforation command overrides the front panel Bottom 
	 margin setting.
	*PANEL LOCK in the Function mode affects this command.

<TOP OF FORM>
Sets current paper position as the new top of form.

	Name:   ESC     4
	Dec.:   27      52
	Hex.:   1B      34

<HORIZONTAL TAB STOP SETTING>
Sets horizontal tabulations to specified values.

	Set:
	Name:   ESC     D       n1      n2...nx         0
	Dec.:   27      68      n1      n2...nx         0
	Hex.:   1B      44      n1      n2...nx         00

	Release:
	Name:   ESC     D       0
	Dec.:   27      68      0
	Hex.:   1B      44      00

	Comments:
	*Horizontal tabs are set from the left margin position.
	*Horizontal tabs must be designated such that n1<n2...<nx.
	*A maximum of 32 tabs may be set on a single line.
	*ESC+D+n1+n2+...+nx+0 sets horizontal tab stops.
	*The HT command executes the tab designation.
	*In proportional spacing, horizontal tabs are set based on 10 CPI.
	*If the character pitch is altered after designation of
	 horizontal tabs, the tab positions change.
	*When the left margin is changed, horizontal tabs will be
	 moved based on the new margin setting.
	*When the printer is powered up, tabs are automatically set
	 every 8 characters.

<HORIZONTAL TAB EXECUTION>
Executes the horizontal TAB as designated by ESC+D+n1+n2+...nx+0.

	Name:   HT
	Dec.:   9
	Hex.:   09

	Comments:
	*If the value of the horizontal TAB is less than the
	 present column position, that HT is ignored.
	*When in underline mode, the blank spaces between
	 consecutive HT print positions are not underlined.

<VERTICAL TAB STOP SETTING>
Sets vertical tabulation to specified values.

	Set:
	Name:   ESC     B       n1      n2...nx         0
	Dec.:   27      66      n1      n2...nx         0
	Hex.:   1B      42      n1      n2...nx         00

	Release:
	Name:   ESC     B       0
	Dec.:   27      66      0
	Hex.:   1B      42      00

	Comments:
	*VT is set from the top of form position.
	*Vertical tabs must be designed such that n1<n2...<nx.
	*ESC+B+n1+n2+...nx+0 sets vertical tab stops. The VT command
	 executes the tab designation.
	*If the paper feed amount is changed after a designation of
	 vertical tabs, the tab positions do not change.
	*A maximum of 64 tabs may be set.

<VERTICAL TAB EXECUTION>
Executes the vertical TAB as designated by ESC+B+n1+n2+...+nx+0.

	Name:   VT
	Dec.:   11
	Hex.:   0B

	Comments:
	*When TABs are set with VT setting command and there is
	 no tab setting on a position exceeding the present line,
	 data in the line buffer is printed and the paper is fed
	 one line (same as LF).
	*When vertical TAB has not been set by ESC+B+n1+n2+...+nx+0,
	 execution of VT causes data in the line buffer to be printed
	 and advances the paper one line (same function as LF).

<ALL TAB INITIAL CLEAR>
Sets all tabs to power on settings.

	Name:   ESC     R
	Dec.:   27      82
	Hex.:   1B      52

	Comment:
	*This command sets horizontal tabs at every 8th position
	 and clears all vertical tabs.

<BACKSPACE>
Prints data in the line buffer and backspaces one space.

	Name:   BS
	Dec.:   8
	Hex.:   08

	Comment:
	*The backspacing amount will depend upon the pitch set when
	 the BS code is executed.

<CARRIAGE RETURN>
Prints all data in the line buffer and returns the printhead
to the left margin position.

	Name:   CR
	Dec.:   13
	Hex.:   0D

	Comments:
	*Certain computers issue an automatic line feed with
	 a carriage return. Check your computer manual for details.
	*When Auto LF is set to ON through the Function mode or 
	 the initial setup mode, a Line Feed command (LF) is added to 
	 each Carriage Return (CR) double width printing set.

<UNI-DIRECTION>
Sets uni-directional printing mode.

	Set:
	Name:   ESC     U       1
	Dec.:   27      85      1
	Hex.:   1B      55      01

	Release:
	Name:   ESC     U       0
	Dec.:   27      85      0
	Hex.:   1B      55      00

	Comment:
	*PANEL LOCK in the Function mode affects this command.

<RELATIVE HORIZONTAL POSITION>
Moves the printhead toward the right n/120 inch.

	Name:   ESC     d       n1      n2
	Dec.:   27      100     n1      n2
	Hex.:   1B      64      n1      n2

	Comments:
	*Each unit equals n/120 of an inch
	*Let m=# of units
		Divide m by 256 using long division
		The quotient=n2
		The remainder=n1
	*When underlining or overlining, spaces created by the move
	 are underlined or overlined.

<CANCEL>
Clears all data in the line buffer.

	Name:   CAN
	Dec.:   24
	Hex.:   18

<REMOTE PRINTER SELECT>
Selects printer after it has been deselected by ESC+Q+36.

	Name:   DC1     (Device Control 1)
	Dec.:   17
	Hex.:   11

	Comment:
	*All data sent to the printer between ESC+Q+36 and DC1 is lost.

<REMOTE DESELECT PRINTER>
Deselects printer until it has been selected by DC1.

	Name:   ESC     Q       36
	Dec.:   27      81      36
	Hex.:   1B      51      24

	Comment:
	*All data sent to the printer between DC3 and DC1 is lost.

<FONT DOWNLOADING>
Defines download characters into specified address locations
in RAM.

	Name:   ESC     =       n1      n2      35      A1      A2      Data
	Dec.:   27      61      n1      n2      35      A1      A2      Data
	Hex.:   1B      3D      n1      n2      23      A1      A2      Data

	Comments:
	*The values n1 and n2 indicate the number of data bytes to be
	 downloaded.
	*The values A1 and A2 are the low order and high order address
	 location of the character being defined.
	*When n1=n2=0, all previously downloaded characters are cleared.
	*PANEL LOCK in the Function mode affects this command
	*This command is operational only when through Function mode 
	 or setup disk
	 Draft and Letter Quality (LQ) fonts can be downloaded simultaneously.
	 Draft download characters are printed when the printer is 
	 in draft mode. LQ characters are printed when the printer is 
	 in LQ mode.
	*Making Maximum Use of the Buffer:
	 IBM mode:
	 The 32K bytes available can be divided between draft and LQ
	 characters in any combination. The download data also can be
	 entered to RAM by compression. The maximum number of characters
	 depends on the manner in which the characters are entered.

	*Entering Download Data
	 IBM mode:

	 Downloading fonts in IBM mode requires downloading character Dot
	 Pattern data and character Index Table data. Dot pattern data
	 controls which pins fire when printing a character. Index Table
	 data is placed in a "look-up table" that provides information on
	 where Dot Pattern data is stored in memory and defines certain
	 attributes of the character.

	 The format for the command to input download data is:
		ESC+"="+n1+n2+35+A1+A2+d1+d2+...+dx
	 where
		n1+(256 x n2)=the number of data bytes to be downloaded, 
		35 is a fixed number that must always be sent, A1h and A2h 
		indicate the low order and high order addresses in which 
		data is to be stored, and d1, d2...is the data being 
		downloaded. This data will be in one of two formats, 
		depending on whether it is Dot Pattern or Index Table:

	 1. Index Table Addresses
	 Starting memory addresses for Index Tables are:
		Draft (10 and 12 CPI)           8011HEX
		LQ 10 CPI                       8912HEX
		LQ Proportional                 9213HEX
		LQ 12 CPI                       9B14HEX

	 To calculate the address for an individual character Index Table
	 Entry, use equation:

	 Address=9 x ASCII character number+starting address.

	 To find the address of the Index Table location for the draft
	 letter "A":
		Multiply 9 x 65 (ASCII character number for "A")=585DEC
		Convert to hexadecimal=249HEX
		Add starting address for draft=8011HEX
		yielding 825AHEX making A1=5AHEX, and A2=82HEX.

	 2. Dot Pattern Data
		Dot Pattern data is sent for all columns that must be 
		uniquely defined. If adjacent horizontal columns are 
		identical (or can be made identical knowing that the 
		printer will not print adjacent horizontal dots) data 
		compression may be used and the duplicate data need not 
		be sent. Dot Pattern data may be stored at any address 
		from A414HEX to FFFFHEX inclusive.

		Dot columns for characters are as follows:
			Draft (10 and 12 CPI)   10 columns
			LQ 10 CPI               36 columns
			LQ 12 CPI               30 columns
			LQ Proportional         18-42 columns

		It is important to note that the last column is always 
		blank. (e.g. A download draft character is defined by 9 
		columns. The printer automatically adds the tenth column.)

			Data=P1H+P1M+P1L+P2H+P2M+P2L+...+PnH+PnM+PnL

	 3. Index Table Data
		AA1+AA2+IT1+IT2+CM1+...+CM5
	 where
		AA1 and AA2 indicate the address where Dot Pattern data 
		is stored.
		AA1 and AA2 are the high order and the low order bytes 
		respectively.

	 IT1 is Index Table byte #1. Bit designation is:

		Bit             0                       1
		7       Normal Character        Graphic Character
		6       Download Character      Resident Character
		5 to 0  Number of columns in the character memory

	 IT2 is Index Table byte #2. Bit designation is:

		Bits 7, 6       Type of block graphic character
				00              shading character
				01              line drawing character
				10              underscore character
				11              not supported

		Bits 5 to 0     number of columns in the character less 1
				[e.g. for draft characters,
				10-1=9DEC=(001001)BIN bits 5 to 0=001001]

	 From CM1 to CM5 are compression mask bits. (0=no compression,
	 1=compression)

		CM1     bit 7=1st dot column
			bit 6=2nd dot column
			.
			.
			.
		CM5     bit 3=37th dot column
			bit 2=38th dot column
			bit 1=39th dot column
			bit 0=40th dot column

	 All block graphic characters are 30 dots high, even though only
	 24 dots are defined for each column. An underline is defined as
	 a blank block graphic character (all zeros). The underline is
	 generated by the printer during the second pass. A shadow character
	 repeats dots 1 to 6 of each column as dots 25 through 30
	 respectively. A line draw character repeats dots 23 and 24 as the
	 pairs 25 and 26, 27 and 28, and 29 and 30.

	 Entry data can designate any character data image whether resident
	 or downloaded. Multiple table entries can designate the same
	 character. The address of an undefined entry should be 000. An
	 undefined entry is printed as a space.

	 Location 0 (00HEX) normally stores the slashed zero. If a character
	 is downloaded into this location, when the slashed zero is selected
	 through the initial setup disk, the downloaded character will print
	 in place of any zero.

	 4. Data Compression
	 Data Compression allows the efficient use of memory in storing
	 downloaded characters, providing space for more characters than
	 would be available without compression. The printer repeats the
	 previous dot column in the current column when the current column
	 compression mask bit is set to 1.

	 5. Resetting Download Area
	 Issuing the command ESC+"="+0+0 initializes the download area.
	 All previously downloaded characters are cleared and the Index
	 Tables are loaded with information for resident fonts.

	 6. Programming Examples:
	 To load the draft character used in the example for the Epson
	 mode (Greek gamma), the following program may be used.

	 10 REM Greek Gamma Character Download and print
	 20 WIDTH "LPT1:",255
	 30 OPEN "LPT1:" AS #1
	 40 REM---(Initialize the Download Buffer)
	 50 PRINT #1,CHR$(27)+"="+CHR$(0)+CHR$(0);
	 60 REM---(Dot Pattern Data Entry to ASCII "A")
	 70 PRINT #1,CHR$(27)+"="+CHR$(30)+CHR$(0)+CHR$(35);
	 80 PRINT #1,CHR$(&H0)+CHR$(&HB0);
	 90 PRINT #1,CHR$(0)+CHR$(128)+CHR$(0);
	 100 PRINT #1,CHR$(1)+CHR$(0)+CHR$(0);
	 110 PRINT #1,CHR$(0)+CHR$(128)+CHR$(0);
	 120 PRINT #1,CHR$(0)+CHR$(65)+CHR$(64);
	 130 PRINT #1,CHR$(0)+CHR$(18)+CHR$(16);
	 140 PRINT #1,CHR$(0)+CHR$(5)+CHR$(64);
	 150 PRINT #1,CHR$(0)+CHR$(16)+CHR$(0);
	 160 PRINT #1,CHR$(1)+CHR$(64)+CHR$(0);
	 170 PRINT #1,CHR$(0)+CHR$(0)+CHR$(0);
	 180 REM---(Index Table Entry to ASCII "A")
	 190 PRINT #1,CHR$(27)+"="+CHR$(12)+CHR$(0)+CHR$(35);
	 200 PRINT #1,CHR$(&H5A)+CHR$(&H82);
	 210 PRINT #1,CHR$(&HB0)+CHR$(&H0)+CHR$(8);
	 220 PRINT #1,CHR$(10)+CHR$(0)+CHR$(0);
	 230 PRINT #1,CHR$(0)+CHR$(0)+CHR$(0);
	 240 REM---(Download Character print)
	 250 PRINT #1,CHR$(27)+"I"+CHR$(4);
	 260 FOR I=1 TO 10
	 270 PRINT #1,"A";
	 280 NEXT
	 290 PRINT #1,CHR$(13);CHR$(10);
	 300 CLOSE #1
	 310 END

	 In this example of Greek gamma, a character is not compressed,
	 and data of CM1 through CM5 are all zeros.

	 To load the LQ character used in the example for the one-eighth-
	 note character, the following program may be used.

	 Input format is the same as with draft fonts.

	 Programming example for the one-eighth-note character is as follows:

	 10 REM One-eight-note Character Download and print
	 20 WIDTH "LPT1:",255
	 30 OPEN "LPT1:" AS #1
	 40 REM---(Initialize the Download Buffer)
	 50 PRINT #1,CHR$(27)+"="+CHR$(0)+CHR$(0);
	 60 REM---(Dot Pattern Data Entry to ASCII "B")
	 70 PRINT #1,CHR$(27)+"="+CHR$(45)+CHR$(0)+CHR$(35);
	 80 PRINT #1,CHR$(&H0)+CHR$(&HB0);
	 90 PRINT #1,CHR$(0)+CHR$(0)+CHR$(0);
	 100 PRINT #1,CHR$(0)+CHR$(0)+CHR$(128);
	 110 PRINT #1,CHR$(0)+CHR$(1)+CHR$(64);
	 120 PRINT #1,CHR$(0)+CHR$(3)+CHR$(224);
	 130 PRINT #1,CHR$(0)+CHR$(7)+CHR$(240);
	 140 PRINT #1,CHR$(0)+CHR$(3)+CHR$(224);
	 150 PRINT #1,CHR$(0)+CHR$(1)+CHR$(64);
	 160 PRINT #1,CHR$(63)+CHR$(254)+CHR$(128);
	 170 PRINT #1,CHR$(14)+CHR$(0)+CHR$(0);
	 180 PRINT #1,CHR$(6)+CHR$(0)+CHR$(0);
	 190 PRINT #1,CHR$(3)+CHR$(0)+CHR$(0);
	 200 PRINT #1,CHR$(1)+CHR$(132)+CHR$(0);
	 210 PRINT #1,CHR$(0)+CHR$(120)+CHR$(0);
	 220 PRINT #1,CHR$(0)+CHR$(0)+CHR$(0);
	 230 REM---(Index Table Entry to ASCII "B")
	 240 PRINT #1,CHR$(27)+"="+CHR$(12)+CHR$(0)+CHR$(35);
	 250 PRINT #1,CHR$(&H64)+CHR$(&H8B);
	 260 PRINT #1,CHR$(&HB0)+CHR$(&H0)+CHR$(14);
	 270 PRINT #1,CHR$(35)+CHR$(124)+CHR$(90);
	 280 PRINT #1,CHR$(85)+CHR$(47)+CHR$(240);
	 290 REM---(Download Character print)
	 300 PRINT #1,CHR$(27)+"I"+CHR$(6);
	 310 FOR I=1 TO 10
	 320 PRINT #1,"B";
	 330 NEXT
	 340 PRINT #1,CHR$(13);CHR$(10);
	 350 CLOSE #1
	 360 END

	 Note:
	 The left most column of adjacent identical columns has its
	 compression mask bit set to 0, and that bit in the other columns
	 is set to 1.

	 Entry data can designate any character data image whether resident
	 or downloaded. Multiple table entries can designate the same
	 character. The address of an undefined entry should be 000.
	 An undefined entry is printed as a space.

	 Location 0 (00HEX) normally stores the slashed zero. If a character
	 is downloaded into this location, when the slashed zero is selected
	 through the initial setup disk, the downloaded character will print
	 in place of any zero.

	 ASCII character in location 255 (FFHEX) cannot be defined.

<BELL>
Sounds the buzzer for approximately 0.5 second.

	Name:   BEL
	Dec.:    7
	Hex.:   07

<ALL CHARACTER CHART PRINTING (Continuous)>
Prints continuously from the All Character Chart.

	Name:   ESC     \       n1      n2
	Dec.:   27      92      n1      n2
	Hex.:   1B      5C      n1      n2

	Comments:
	*The values specified for n1 and n2 indicate how many
	 characters to print from All Character Chart, calculating
	 the total count with this formula; Total count=n2x256+n1.
	*The data following this command will be printed as characters
	 from the All Character Chart.
	*Refer to IBM All Character Chart in appendix of the operating
	 instruction manual.

<ALL CHARACTER CHART PRINTING (Single)>
Prints a single character from the All Character Chart.

	Name:   ESC     ^
	Dec.:   27      94
	Hex.:   1B      5E

	Comments:
	*Only the first byte of data following this command will
	 be printed as a character from the All Character Chart.
	*Refer to IBM All Character Chart in appendix of the operating
	 instruction manual.

<SETS OFF LINE MODE>
Stops printing and sets printer to OFF LINE mode.

	Name:   ESC     j
	Dec.:   27      106
	Hex.:   1B      6A

	Comment:
	*When you desire to print again, press the ON LINE switch.

<INITIAL STATE>
Resets to initial state.

	Name:   ESC  [    K    n1   0    m   36   p1   p2
	Dec.:   27   91   75   n1   0    m   36   p1   p2
	Hex.:   1B   5B   4B   n1   00   m   24   p1   p2

	Comments:
	*The following values of n1 can be used.
		n1=1: Initialize only
		n1=3: Initialize and set by p1
		n1=4: Initialize and set by p1 and p2
	*The following table illustrates the various modes based
	 upon the value of m.

	m       Initialization          Download
	---------------------------------------------------------
	0       Current setting         Not cleared     Not saved
	1       Current setting         Cleared         Not saved
	4       FACTORY setting         Not Cleared     Not saved
	5       FACTORY setting         Cleared         Not saved
	254     Current setting         Cleared         Saved
	255     FACTORY setting         Cleared         Saved

	*The following tables illustrate the parameter specifications.

	p1 (Parameter 1)
	Bit                  OFF                 ON
	----------------------------------------------------------
	7  Discard byte      Process this byte   Ignore this byte
	6  Not used
	5  Paper out alarm   Enable              Disable
	4  Auto CR           OFF                 ON
	3  Auto LF           OFF                 ON
	2  Form length       11"		 12"
	1  Zero slash        Normal              Slashed Zero
	0  Character set     Set 1               Set 2

	p2 (Parameter 2):
	Bit                  OFF                 ON
	----------------------------------------------------------
	7  Discard byte      Process this byte   Ignore this byte
	6  Select code page  USA                 Multilingual
	5  Not used          ---                 ---
	4  Not used          ---                 ---
	3  Not used          ---                 ---
	2  Not used          ---                 ---
	1  Not used          ---                 ---
	0  Cut sheet feeder  Disable             Enable


<PRINT COLOR>
Select printing color

	SET :
	NAME:   ESC    r     n    
	Dec.:   27     114   n    
	Hex.:   1B     72    n    

	Comment:
	*The following values of n can be used:
		n=0     Black
		n=1     Red (Magenta)
		n=2     Blue (Cyan)
		n=3     Violet
		n=4     Yellow
		n=5     Orange (Red)
		n=6     Green

	Notes:
	*This command is operational only when the color kit (KX-PC11) is 
	 installed.
	*Print yellow first when overlapping colors.

< IBM Mode Characters (USA)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0  30  30  30  30  30  36  30  36  42  36  30  30  30  30  30  30

     1  1  30  30  30  30  42  42  30  36  36  42  18  30  30  30  36  30

     2  2  30  30  30  30  42  42  36  30  30  42  30  30  30  30  36  30

     3  3  30  30  30  30  42  36  30  30  30  30  36  30  30  30  36  30

     4  4  30  30  30  30  42  42  36  24  30  30  36  30  30  30  42  30

     5  5  30  30  30  30  36  42  30  36  30  30  42  30  30  30  36  30

     6  6  30  30  36  30  36  42  24  36  30  36  30  30  30  30  36  30

     7  7  30  30  18  30  42  42  36  42  30  36  30  30  30  30  30  30

     8  8  30  30  30  30  42  42  36  36  30  36  30  30  30  30  42  30

     9  9  30  30  30  30  24  42  18  36  30  42  30  30  30  30  42  30

    10  A  30  30  30  30  30  36  18  30  30  42  30  30  30  30  42  30

    11  B  30  30  30  30  42  30  36  30  18  30  30  30  30  30  30  30

    12  C  30  30  30  30  36  30  18  30  18  30  30  30  30  30  30  30

    13  D  30  30  30  30  42  30  42  30  18  30  30  30  30  30  42  30

    14  E  30  30  30  30  42  30  36  30  42  42  42  30  30  30  30  30

    15  F  30  30  30  30  42  30  30  30  42  30  42  30  30  30  30  30

	Compressed PS width is 1/2 of Normal PS.
					    Unit:1/360 inch (0.07 mm)


< IBM Mode Characters (Multilingual)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0  30  30  30  30  30  36  30  36  42  36  30  30  30  36  42  30

     1  1  30  30  30  30  42  42  30  36  36  42  18  30  30  42  36  30

     2  2  30  30  30  30  42  42  30  30  30  42  30  30  30  36  42  30

     3  3  30  30  30  30  42  36  30  30  30  30  36  30  30  36  42  30

     4  4  30  30  30  30  42  42  36  24  30  30  36  30  30  36  30  30

     5  5  30  30  36  30  36  42  30  36  30  30  42  42  30  18  42  30

     6  6  30  30  36  30  36  42  24  36  30  36  30  42  30  24  36  30

     7  7  30  30  18  30  42  42  36  42  30  36  30  42  42  24  36  30

     8  8  30  30  30  30  42  42  36  36  30  36  30  30  30  24  42  30

     9  9  30  30  30  30  24  42  18  36  30  42  30  30  30  30  42  30

    10  A  30  30  30  30  30  36  18  30  30  42  30  30  30  30  42  30

    11  B  30  30  30  30  42  30  36  30  18  30  30  30  30  30  42  30

    12  C  30  30  30  30  36  30  18  30  18  30  30  30  30  30  36  30

    13  D  30  30  30  30  42  30  42  30  18  42  30  30  30  30  42  30

    14  E  30  30  30  30  42  30  36  30  42  30  42  30  30  24  30  30

    15  F  30  30  30  30  42  30  30  30  42  30  42  30  30  30  30  30

	Compressed PS width is 1/2 of Normal PS.
					    Unit:1/360 inch (0.07 mm)


< IBM Mode Characters (Portugal)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0  30  30  30  30  30  36  30  36  42  36  30  30  30  30  30  30

     1  1  30  30  30  30  42  42  30  36  36  42  18  30  30  30  36  30

     2  2  30  30  30  30  42  42  36  30  30  36  30  30  30  30  36  30

     3  3  30  30  30  30  42  36  30  30  30  30  36  30  30  30  36  30

     4  4  30  30  30  30  42  42  36  24  30  30  36  30  30  30  42  30

     5  5  30  30  36  30  36  42  30  36  30  30  42  30  30  30  36  30

     6  6  30  30  36  30  36  42  24  36  42  42  30  30  30  30  36  30

     7  7  30  30  18  30  42  42  36  42  30  36  30  30  30  30  30  30

     8  8  30  30  30  30  42  42  36  30  30  24  30  30  30  30  42  30

     9  9  30  30  30  30  24  42  18  36  36  42  42  30  30  30  42  30

    10  A  30  30  30  30  30  36  18  30  30  42  30  30  30  30  42  30

    11  B  30  30  30  30  42  30  36  30  24  30  30  30  30  30  30  30

    12  C  30  30  30  30  36  30  18  30  42  30  30  30  30  30  30  30

    13  D  30  30  30  30  42  30  42  30  18  42  30  30  30  30  42  30

    14  E  30  30  30  30  42  30  36  30  42  42  42  30  30  30  30  30

    15  F  30  30  30  30  42  30  30  30  42  42  42  30  30  30  30  30

	Compressed PS width is 1/2 of Normal PS.
					    Unit:1/360 inch (0.07 mm)


< IBM Mode Characters (Canada-French)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0  30  30  30  30  30  36  30  36  42  36  30  30  30  30  30  30

     1  1  30  30  30  30  42  42  30  36  36  36  30  30  30  30  36  30

     2  2  30  30  30  30  42  42  36  30  30  36  30  30  30  30  36  30

     3  3  30  30  30  30  42  36  30  30  30  30  36  30  30  30  36  30

     4  4  30  30  30  30  42  42  36  24  42  36  30  30  30  30  42  30

     5  5  30  30  30  30  36  42  30  36  30  24  30  30  30  30  36  30

     6  6  30  30  36  30  36  42  24  36  30  36  30  30  30  30  36  30

     7  7  30  30  18  30  42  42  36  42  30  36  30  30  30  30  30  30

     8  8  30  30  30  30  42  42  36  36  30  30  24  30  30  30  42  30

     9  9  30  30  30  30  24  42  18  36  30  42  30  30  30  30  42  30

    10  A  30  30  30  30  30  36  18  30  30  42  30  30  30  30  42  30

    11  B  30  30  30  30  42  30  36  30  18  30  30  30  30  30  30  30

    12  C  30  30  30  30  36  30  18  30  18  30  30  30  30  30  30  30

    13  D  30  30  30  30  42  30  42  30  30  42  30  30  30  30  42  30

    14  E  30  30  30  30  42  30  36  30  42  42  42  30  30  30  30  30

    15  F  30  30  30  30  42  30  30  30  30  30  42  30  30  30  30  30

	Compressed PS width is 1/2 of Normal PS.
					    Unit:1/360 inch (0.07 mm)


< IBM Mode Characters (Norway)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0  30  30  30  30  30  36  30  36  42  36  30  30  30  30  30  30

     1  1  30  30  30  30  42  42  30  36  36  42  18  30  30  30  36  30

     2  2  30  30  30  30  42  42  36  30  30  42  30  30  30  30  36  30

     3  3  30  30  30  30  42  36  30  30  30  30  36  30  30  30  36  30

     4  4  30  30  30  30  42  42  36  24  30  30  36  30  30  30  42  30

     5  5  30  30  30  30  36  42  30  36  30  30  42  30  30  30  36  30

     6  6  30  30  36  30  36  42  24  36  30  36  30  30  30  30  36  30

     7  7  30  30  18  30  42  42  36  42  30  36  30  30  30  30  30  30

     8  8  30  30  30  30  42  42  36  36  30  36  30  30  30  30  42  30

     9  9  30  30  30  30  24  42  18  36  30  42  30  30  30  30  42  30

    10  A  30  30  30  30  30  36  18  30  30  42  30  30  30  30  42  30

    11  B  30  30  30  30  42  30  36  30  18  30  30  30  30  30  30  30

    12  C  30  30  30  30  36  30  18  30  18  30  30  30  30  30  30  30

    13  D  30  30  30  30  42  30  42  30  18  42  30  30  30  30  42  30

    14  E  30  30  30  30  42  30  36  30  42  42  42  30  30  30  30  30

    15  F  30  30  30  30  42  30  30  30  42  30  30  30  30  30  30  30

	Compressed PS width is 1/2 of Normal PS.
					    Unit:1/360 inch (0.07 mm)


< IBM Mode Characters (Turkey)>

    Dec.    0  16  32  48  64  80  96 112 128 144 160 176 192 208 224 240

       Hex. 0   1   2   3   4   5   6   7   8   9   A   B   C   D   E   F

     0  0  30  30  30  30  30  36  30  36  42  36  30  30  30  30  30  30

     1  1  30  30  30  30  42  42  30  36  36  42  18  30  30  30  36  30

     2  2  30  30  30  30  42  42  36  30  30  42  30  30  30  30  36  30

     3  3  30  30  30  30  42  36  30  30  30  30  36  30  30  30  36  30

     4  4  30  30  30  30  42  42  36  24  30  30  36  30  30  30  42  30

     5  5  30  30  30  30  36  42  30  36  30  30  42  30  30  30  36  30

     6  6  30  30  36  30  36  42  24  36  30  36  42  30  30  30  36  30

     7  7  30  30  18  30  42  42  36  42  30  36  36  30  30  30  30  30

     8  8  30  30  30  30  42  42  36  36  30  24  30  30  30  30  42  30

     9  9  30  30  30  30  24  42  18  36  30  42  30  30  30  30  42  30

    10  A  30  30  30  30  30  36  18  30  30  42  30  30  30  30  42  30

    11  B  30  30  30  30  42  30  36  30  30  30  30  30  30  30  30  30

    12  C  30  30  30  30  36  30  18  30  18  30  30  30  30  30  30  30

    13  D  30  30  30  30  42  30  42  30  18  30  30  30  30  30  42  30

    14  E  30  30  30  30  42  30  36  30  42  36  42  30  30  30  30  30

    15  F  30  30  30  30  42  30  30  30  42  30  42  30  30  30  30  30

	Compressed PS width is 1/2 of Normal PS.
					    Unit:1/360 inch (0.07 mm)
