COM154 V1.0
879 ,  905 
906 ,  930 
931 ,  957 
958 ,  983 
984 ,  1015 
1016 ,  1044 
1045 ,  1067 
1068 ,  1099 
1100 ,  1124 
1125 ,  1154 
1155 ,  1242 
1243 ,  1249 
1250 ,  1276 
1277 ,  1456 
1457 ,  1485 
1486 ,  1583 
1584 ,  1630 
1631 ,  1721 
1722 ,  1748 
1749 ,  1776 
1777 ,  1832 
1833 ,  2072 
2073 ,  2298 
2299 ,  2325 
2326 ,  2351 
2352 ,  2376 
2377 ,  2403 
2404 ,  2432 
2433 ,  2460 
2461 ,  2483 
2484 ,  2506 
2507 ,  2528 
2529 ,  2553 
2554 ,  2596 
2597 ,  2603 
2604 ,  2696 
2697 ,  2943 
2944 ,  2990 
2991 ,  3021 
3022 ,  3065 
3066 ,  3087 
3088 ,  3121 
3122 ,  3249 
3250 ,  3345 
3346 ,  3369 
3370 ,  3425 
3426 ,  3625 
3626 ,  3793 
3794 ,  3851 
3852 ,  3876 
3877 ,  3903 
3904 ,  3928 
3929 ,  3950 
3951 ,  3974 
3975 ,  4016 
4017 ,  4061 
4062 ,  4092 
4093 ,  4122 


<
Select print style


<
Select emulation


<
Select page format


<
Select print mode


<
Select text enhancement


<
Select character set


<
Select install


<
Select display language


<
Select interface


<
Select power on macro


<
Select font style
Style of typeface.
                  
SC is SCALABLE FONT.


<


<
Select point size.


<
Select emulation
Allows KX-P3124 to operate like another printer.Be sure to select a printer     driver in your application software that supports the emulation selected.


<
Select line per inch


<
Select page length
Top to bottom measurement of a page. Allows for correct form feeding.


<
Select top margin
1st print position.


<
Select bottom margin
The area from the last print line to the bottom of the page.


<
Select left margin


<
Select right margin


<
Select new center point location for printhead.


<
Select graphic direction
Select uni-directional or bi-directional graphic printing
Prints graphics left to right only (UNI), permits better vertical alignment.
Prints graphics in both directions (BI), increases processing speed.


<
Select text direction
Select uni-directional or bi-directional text printing
Prints text left to right only (UNI), permits better vertical alignment.
Prints text in both directions (BI), increases processing speed.


<
Select print width


<
Select panel lock


<
Select bold mode


<
Select double high


<
Select double strike


<
Select double width


<
Select italics


<
Select outline


<
Select shadow


<
Select zero font


<
Select international character set


<


<
Select code page
The set of characters, numbers and symbols available for printing.


<
Set or release the alternate graphic mode - for IBM mode only
Graphic printing command Esc+* is effective and prints 8 pin graphic modes 
using all 24 pins and changes vertical line spacing amount of Esc+J+n,
Esc+A+n, and Esc+3+n (ON).


<
Select auto carriage return (IBM ONLY)


<
Select auto line feed.


<
Select auto loading (FRICTION ONLY)


<
Select buzzer


<
Select paper out detector


<
Select or release super quiet mode
When ON, printing noise will be reduced, however, print speed will
also be slower.


<
Select REV LF (reverse line feed)
This can only be used when in the Pull Tractor mode.


<
Select tear off


<
Activate your cut sheet feeder - when installed


<
Enable or disable download buffer
Sections off a portion of the buffer to be used for the custom design of
special characters (ON) or allows entire buffer to be used for data
memory (OFF).


<
The feature is available with the optional color kit installed.
Each of the three colors can be mixed (7 colors max.) through
your setup disk or front panel.


<
Select language to be displayed on printer's LCD.


<
Select interface


<
Select data length


<
Select baud rate


<
Select parity


<
Select protocol


<
Select resume data transfer (RDT)


<
Select suspended data transfer (SDT)


<
Select signal polarity


<
Select power on macro


