##B **00-01

##Y one
{
 &&hercs &&herctl !!SIBM0HER-SIBM1HET
 &&herss &&herlad !!SIBM0H1B-SIBM1H1S
 &&colcs &&colcl !!SIBM0B&W-SIBM1HRT
 &&ibms &&ibmtl !!SIBM0COL-SIBM1MRT
 &&plas &&platl !!SIBM0COL-SIBM1PMT
 &&egas &&egatl !!SIBM0EGT-SIBM1EGT
 &&attb &&atttl !!SIBM0B&W-SATT1HRT
 &&attc &&atttcl !!SIBM0COL-SIBM1MRT
 &&att &&attsl !!SATT0MBT-SATT1HRT
 &&3270pcc &&3270pccl !!SIBM0COL-S32_1MRT
 &&3270pc &&3270pcl !!S32_0MO-S32_1HRT
 &&3270gx &&3270gxtl !!SIBM0COL-SGX1MRT
 &&comps &&comptl !!SIBM0CPQ-SIBM1HRT
 &&compc &&comptc !!SIBM0COL-SIBM1MRT
 &&pcs &&pctl !!SIBM0B&W-SIBM1HRT
 &&tecbws &&stecbwl !!1T-1G
 &&teccols &&steccoll !!2T-1G
}

##Y dual
{
 &&ibms &&duall !!SIBM0MON-SIBM1MRD
 &&egduals &&egduall !!SIBM0MON-SIBM1EGD
 &&tecbws &&dtecbwl !!SIBM0MON-3G
 &&teccols &&dteccoll !!SIBM0MON-3G
}

***************** SHORT PROMPTS ************

&&attc
{
AT&T 6300, color monitor
}
&&attb
{
AT&T 6300, single-color monitor
}
&&att
{
AT&T 6300 (80 x 50)
}
&&colcs
{
IBM color card, single-color monitor
}
&&egas
{
Enhanced Graphics Adapter
}
&&hercs
{
Hercules card (80 x 25)
}
&&herss
{
Hercules card (90 x 38)
}
&&pcs
{
IBM Portable Computer
}
&&comps
{
COMPAQ, single-color monitor
}
&&compc
{
COMPAQ, color monitor
}
&&egduals
{
IBM Enhanced Graphics Adapter
}
&&ibms
{
IBM color card
}
&&plas 
{
Plantronics ColorPlus card
}
&&3270pc
{
IBM 3270-PC, monochrome monitor
}
&&3270pcc
{
IBM 3270-PC, color monitor
}
&&3270gx 
{
IBM 3270-PC/GX
}
&&tecbws
{
Tecmar GM card, single-color monitor
}
&&teccols
{
Tecmar GM card, color monitor
}

************* LONG PROMPTS ****************

&&egatl
{
Select this for any kind of
monitor and an IBM Enhanced
Graphics Adapter.
}
&&attsl
{
Select this for an AT&T 6300
with a single-color or color 
graphics monitor. This option
lets you see more of the 1-2-3 
work area than you can using 
the standard display. Text is
smaller and operations are 
slower. This choice does NOT 
permit you to run the View of 
1-2-3 and is NOT recommended
for use with the Tutorial.
}
&&atttl
{
Select this for an AT&T 6300
with a single-color graphics 
monitor if you want a standard 
80 x 25 screen display.
}
&&atttcl
{
Select this for an AT&T 6300
with a color monitor if you 
want a standard 80 x 25 
screen display.
}
&&herctl
{
Select this for an IBM
monochrome monitor with a
Hercules graphics card if 
you want a standard 80 x 25
screen display.
}
&&herlad
{
Select this for an IBM
monochrome monitor with a
Hercules card if you want to
see more of the 1-2-3 work 
area than you can with the 
80 x 25 display. Text is 
smaller and operations are 
slower. This choice does NOT 
permit you to run the View of
1-2-3 and is NOT recommended 
for use with the Tutorial.
}
&&pctl
{
Select this for an IBM
Portable Computer.
}
&&comptl
{
Select this for a COMPAQ
computer with a single-color
monitor.
}
&&comptc
{
Select this for a COMPAQ
computer with a color
monitor.
}
&&duall
{
Select this if you have an
IBM color graphics card for
the monitor you are using
to display graphs.
}
&&egduall
{
Select this if you have the
IBM Enhanced Graphics Adapter
for the monitor you are using
to display graphs.
}
&&ibmtl
{
Select this for an IBM color
card connected to a color
monitor, or a PCjr, or an
IBM 3270-PC/G.
}
&&platl
{
Select this for a Plantronics
ColorPlus card connected to
a color monitor.
}
&&egactl
{
Select this for an IBM
Enhanced Graphics Adapter
connected to a color monitor.
}
&&colcl
{
Select this for an IBM color
card connected to a single-
color graphics monitor (for
example, black and white,
black and green, or black
and amber).
}
&&3270pcl
{
Select this for an IBM
3270-PC with a monochrome
monitor.
}
&&3270pccl
{
Select this for an IBM
3270-PC with a color monitor.
}
&&3270gxtl
{
Select this for an
IBM 3270-PC/GX.
}
&&stecbwl
{
Select this if you have
a Tecmar graphics card
connected to a single-color
monitor
}
&&steccoll
{
Select this if you have
a Tecmar graphics card
connected to a color monitor.
}
&&dtecbwl
{
Select this if you have a
Tecmar graphics card connected
to a single-color monitor to
display graphs.
}
&&dteccoll
{
Select this if you have a
Tecmar graphics card connected
to a color monitor to 
display graphs.
}
##E **00-01

