GETTYTAB(5)

NAME
gettytab - terminal configuration data base

SYNOPSIS
/etc/gettytab

DESCRIPTION
The /etc/gettytab file is a simplified version of the termcap(5) data base used to describe terminal lines. The initial terminal login process, getty(8), accesses the /etc/gettytab file each time it starts, allowing reconfiguration of terminal characteristics. Each entry in the data base describes one class of terminals. Init passes the second character of an entry in the /etc/ttys file to getty, which uses this character to select an entry in the /etc/gettytab file.

There is a default terminal class, default, that sets global characteristics for all classes. The default entry is read first. Then the entry for the class required is read, overriding some default settings.

CAPABILITIES
Refer to termcap(5) for a description of the file layout. The default column lists default values that are used when there is no corresponding entry either in the special default table or in the table obtained.
Name	Type	Default	Description
ap	bool	false	terminal uses any parity
bd	num	0	backspace delay
bk	str	0377	alternate end of line character (input break)
cb	bool	false	use crt backspace mode
cd	num	0	carriage-return delay
ce	bool	false	use crt erase algorithm
ck	bool	false	use crt kill algorithm
cl	str	NULL	screen clear sequence
co	bool	false	console - add \n after login prompt
ds	str	^Y	delayed suspend character
ec	bool	false	leave echo OFF
ep	bool	false	terminal uses even parity
er	str	^?	erase character
et	str	^D	end of text (EOF) character
ev	str	NULL	initial environment
f0	num	unused	tty mode flags to write messages
f1	num	unused	tty mode flags to read login name
f2	num	unused	tty mode flags to leave terminal as
fd	num	0	form-feed (vertical motion) delay
fl	str	^O	output flush character
hc	bool	false	do NOT hangup line on last close
he	str	NULL	hostname editing string
hn	str	hostname	hostname
ht	bool	false	terminal has real tabs
ig	bool	false	ignore garbage characters in login name
im	str	NULL	initial (banner) message
in	str	^C	interrupt character
is	num	unused	input speed
kl	str	^U	kill character
lc	bool	false	terminal has lower case
lm	str	login:	login prompt
ln	str	^V	``literal next'' character
lo	str	/bin/login	program to exec when name obtained
nd	num	0	newline (line-feed) delay
nl	bool	false	terminal has (or may have) a newline character
np	bool	false	terminal does not use parity
nx	str	default	next table (for auto speed selection)
op	bool	false	terminal uses odd parity
os	num	unused	output speed
pc	str	\0	pad character
pe	bool	false	use printer (hard copy) erase algorithm
pf	num	0	delay between first prompt and following flush (seconds)
ps	bool	false	line connected to a MICOM port selector
qu	str	^\	quit character
rp	str	^R	line retype character
rw	bool	false	do NOT use raw for input, use cbreak
sp	num	unused	line speed (input and output)
su	str	^Z	suspend character
tc	str	none	table continuation
to	num	0	timeout (seconds)
tt	str	NULL	terminal type (for environment)
ub	bool	false	do unbuffered output (of prompts etc)
uc	bool	false	terminal is known upper case only
we	str	^W	word erase character
xc	bool	false	do NOT echo control chars as ^X
xf	str	^S	XOFF (stop output) character
xn	str	^Q	XON (start output) character

If the line speed is zero or unspecified, speed will not be altered from that which prevails when getty is entered. Specifying an input or output speed will override line speed for stated direction only.

Terminal modes to be used for the output of the message, for input of the login name, and to leave the terminal set as upon completion, are derived from the boolean flags specified. If the derivation should prove inadequate, any (or all) of these three may be overridden with one of the f0, f1, or f2 numeric specifications, which can be used to specify (usually in octal, with a leading '0') the exact values of the flags. Local (new tty) flags are set in the top 16 bits of this (32 bit) value.

Note that using f2 to specify the mode in which to leave the tty is ineffective if the default lo value is used because /bin/login resets the tty mode before prompting for information.

Should getty receive a null character (presumed to indicate a line break) it will restart using the table indicated by the nx entry. If there is none, it will re-use its original table.

Delays are specified in milliseconds, the nearest possible delay available in the tty driver will be used. Should greater certainty be desired, delays with values 0, 1, 2, and 3 are interpreted as choosing that particular delay algorithm from the driver.

The cl screen clear string may be preceded by a (decimal) number of milliseconds of delay required (a la termcap). This delay is simulated by repeated use of the pad character pc.

The initial message, and login message, im and lm may include the character sequence %h to obtain the hostname. (%% obtains a single '%' character.) The hostname is normally obtained from the system, but may be set by the hn table entry. In either case it may be edited with he. The he string is a sequence of characters, each character that is neither '@' nor '#' is copied into the final hostname. A '@' in the he string, causes one character from the real hostname to be copied to the final hostname. A '#' in the he string, causes the next character of the real hostname to be skipped. Surplus '@' and '#' characters are ignored.

When getty execs the login process, given in the lo string (usually "/bin/login"), it will have set the environment to include the terminal type, as indicated by the tt string (if it exists). The ev string, can be used to enter additional data into the environment. It is a list of comma separated strings, each of which will presumably be of the form name=value.

If a non-zero timeout is specified, with to, then getty will exit within the indicated number of seconds, either having received a login name and passed control to login, or having received an alarm signal, and exited. This may be useful to hangup dial-in lines.

Output from getty is even parity unless op is specified. Op may be specified with ap to allow any parity on input, but generate odd parity output. Note: this only applies while getty is being run; terminal driver limitations prevent a more complete implementation. Np may be specified to disable parity output entirely. Getty does not check parity of input characters in RAW mode.

FILES
/etc/gettytab

SEE ALSO
termcap(5), getty(8)
DYNIX System Administration Guide

BUGS
It is wise to always specify (at least) the erase, kill, and interrupt characters in the default table. In all cases, '#' or '^H' typed in a login name will be treated as an erase character, and '@' will be treated as a kill character.