MSG154 V1.0
         *PRINT STYLE
         *EMULATION
         *PAGE FORMAT
         *PRINT MODE
         *TEXT ENHANCEMENT
         *CHARACTER SET
         *INSTALL
         *DISPLAY LANGUAGE
         *INTERFACE
         *POWER ON MACRO
         3,FONT            ,PITCH           ,POINT SIZE
         1,EMULATION
         7,LINE/INCH       ,PAGE LENGTH     ,TOP MARGIN
           BOTTOM MARGIN, LEFT MARGIN, RIGHT MARGIN
           CTR PRINTHEAD
         4,G.DIRECTION     ,T.DIRECTION     ,PRINT WIDTH
           PANEL LOCK
         8,BOLD            ,DOUBLE HIGH     ,DOUBLE STRIKE
           DOUBLE WIDE     ,ITALICS
           OUTLINE         ,SHADOW          ,ZERO FONT
         3,COUNTRY         ,CHARACTER SET   ,CODE PAGE
         12,AGM/IBM         ,AUTO CR/IBM     ,AUTO LF
           AUTO LOADING, BUZZER, P.O.DETECTOR
           QUIET MODE, REV LF/PULL     , TEAR OFF
           CSF MODE, DOWNLOAD        , COLOR
         1,DISPLAY LANGUAGE
         8,INTERFACE       , LENGTH     ,BAUD RATE
           PARITY          ,PROTOCOL        ,RDT             ,SDT
           SIGNAL POLARITY
         1,POWER ON MACRO
         2 ,16,DRAFT, BOLD PS, COURIER,OCR-B, ORATOR,PRESTIGE
               ROMAN,SANS SERIF,SCRIPT,SUPER LQ,BOLD PS SC,COURIER SC
               PRESTIGE SC, ROMAN SC, SANS SERIF SC, SCRIPT SC
            10,10 CPI, 12 CPI, 15 CPI,17 CPI, 20 CPI, PROPORTIONAL
               5 CPI, 6 CPI, 7.5 CPI,8.5 CPI
         1 ,2 ,EPSON, IBM
         1 ,15, 1 LPI,  1.5 LPI,  2 LPI, 2.5 LPI,  3 LPI,  4 LPI, 4.5 LPI,  5 LPI,  6 LPI
                7.5 LPI,  8 LPI,  9 LPI,10 LPI, 12 LPI,SC
         4 ,2 ,UNI, BI
            2 ,BI, UNI
            2 ,8 INCH, 9 INCH
            5 ,OFF, FONT, PITCH,FONT&PITCH, ALL
         8 ,2 ,OFF, ON
            2 ,OFF, ON
            2 ,OFF, ON
            2 ,OFF, ON
            2 ,OFF, ON
            2 ,OFF, ON
            2 ,OFF, ON
            3 ,NORMAL, POINT, SLASH
         3 ,15,DENMARK 1, DENMARK 2,FRANCE,GERMANY,ITALY,JAPAN
               KOREA,L.AMERICA,LEGAL,NORWAY,SPAIN 1,SPAIN 2
               SWEDEN,UK,USA
            3 ,ITALIC, GRAPHIC 1, GRAPHIC 2
            6 ,USA, MULTILINGUAL, PORTUGAL,CANADA FRENCH, NORWAY, TURKEY
         12,2 ,OFF, ON
            2 ,OFF, ON
            2 ,OFF, ON
            2 ,ON, OFF
            2 ,ON, OFF
            2 ,ON, OFF
            2 ,OFF, ON
            2 ,OFF, ON
            2 ,MANUAL, AUTO
            2 ,OFF, ON
            2 ,OFF, ON
            7 ,BLACK, BLUE, GREEN,ORANGE, RED, VIOLET,YELLOW
         1 ,6 ,ENGLISH, FRENCH, GERMAN,SPANISH, ITALIAN,TURKISH
         8 ,2 ,PARALLEL, SERIAL
            2 ,8 BIT, 7 BIT
            7 ,150, 300, 600,1200, 2400, 4800,9600
            4 ,NONE, IGNORE, ODD,EVEN
            2 ,DTR,XON/OFF
            2 ,SDT+128, SDT+256
            2 ,RBC 128, RBC 512
            2 ,MARK, SPACE
         1 ,5 ,#1, #2, #3,#4, FACTORY
         YES,NO
         ALL,CURRENT
         1:   LPT1,2:   LPT2,3:   LPT3,4:   COM1,5:   COM2
         1:   9600,2:   4800,3:   2400,4:   1200,5:    600,6:    300,7:    150
         1:   NONE,2:    ODD,3:   EVEN
         1:   8bit,2:   7bit
         1:    DTR,2: XON/OFF
         YES,NO
         PORT,BAUD RATE,PARITY,DATA LENGTH,PROTOCOL
         F1=HELP,F3=SAVE TO DISK,F5=PRINT SETTINGS
         F2=FACTORY SETTINGS,F4=LOAD FROM DISK,F10=SEND TO PRINTER,ESC=EXIT
         ENTER KEY


